Hi All,

  I have Clarence's C1 door closed/open calibration sequences
implemented in the planning tool.  Below is a summary of the
steps and times required.  Russ is checking with Doug and Chris
as to when would be a good time to run this.

-Scott.



C1 DOOR CLOSED CALIBRATIONS
---------------------------
1. Upload C1 DPT:3 WL/exp tables - 970731door_closed_wlexp_tables.sce
2. Set C1 camera DPT:3 to FFV/Full Res.
3. Close C1 door
4. Take 1 step FeXIV line scan dpt:3 to verify door is closed
5. send 970731door_closed_obs.IPT (with c2/c3/eit images taken between
   C1 filters this should take about 2-3 hours)



C1 DOOR OPEN CALIBRATIONS
-------------------------
The door open calibrations (970731door_open_obs.IPT) can either be 
integrated into the nightly schedule or they could be run during NRT.
I estimate they should take about 3-4 hours again with c2/c3/eit images
taken between C1 filters.
1. Open C1 door
2. Take 1 step FeXIV line scan dpt:3 to verify door is open
3. send 970731door_open_obs.IPT
