DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/bmd2/CDS_STUDY/ar_so_wa_2.def
INSTRUME = CDS
DATE_CRE = 2003/03/31 14:22:24
END

LINELIST
    LL_ID    = 442
    DETECTOR = N
    LL_DESC  = AR-SO-Wavelength-Test
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = SiXII-HeI
        WAVELNTH = 523
        GR_ORDER = 1
        CEN_PIX  = 98
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = SiXI-HeI
        WAVELNTH = 582.6
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2

DATAWIN
    DW_ID    = 569
    DETECTOR = N
    DW_DESC  = 2 lines. {0}  dex = (80,120) pixels <2378>
    W_WIDTH  = 80
    W_HEIGHT = 120
    VDS_BACK = 0
    LL_ID    = 442
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = WW_523_00                               
        WIN_DEF  = (58,392,80,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_582_60                               
        WIN_DEF  = (568,392,80,120)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 76
    RV_DESC  = (240x240) arcsec, 25s <ACTIVE>  Comp. 2 IDs-(442,569)
    EXPTIME  = 25
    LL_ID    = 442
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 569
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3708
    USABLE   = Y

LINELIST
    LL_ID    = 443
    DETECTOR = N
    LL_DESC  = AR-SO-Wavelength-Test2
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = OIV-MgX
        WAVELNTH = 609.1
        GR_ORDER = 1
        CEN_PIX  = 834
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = MgX-OV
        WAVELNTH = 627
        GR_ORDER = 1
        CEN_PIX  = 987
        WAVEBAND = 2

DATAWIN
    DW_ID    = 570
    DETECTOR = N
    DW_DESC  = Background,   2 lines. {0}  dex = (80,120) pixels <8004>
    W_WIDTH  = 80
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 443
    N_WINS   = 6
    DW_IND   = 1
        WIN_NAME = WW_609_10                               
        WIN_DEF  = (794,392,80,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_627_00                               
        WIN_DEF  = (947,392,76,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 77
    RV_DESC  = (240x240) arcsec, 25s <ACTIVE>  Comp. 2 IDs-(443,570)
    EXPTIME  = 25
    LL_ID    = 443
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 570
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3800
    USABLE   = Y

STUDY
    STUDY_ID = 279
    TITLE_ID = 582
    OBS_PROG = AR_SO_WA
    TITLE    = AR/SOLAR-ORBITER/WAVELENGTH-TEST
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 279
    TITLE_ID = 582
    STUDYVAR = 2
    SV_DESC  = AR, 25 S, 2 WINDOWS X2, 2'X240'
    N_RASTERS0 = 1
    DURATION0 = 3800
    DURATION1 = 3800
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 76
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 10
        RAS_VAR  = 77
        N_REPEAT_R = 1
