DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/ccdjar/jar24/blink_te_23.def
INSTRUME = CDS
DATE_CRE = 2006/01/05 17:09:38
END

LINELIST
    LL_ID    = 473
    DETECTOR = N
    LL_DESC  = blink_te lines (4 lines) Madjarska
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = 
        WAVELNTH = 560.284
        GR_ORDER = 1
        CEN_PIX  = 417
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.3
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He II
        WAVELNTH = 607.4
        GR_ORDER = 1
        CEN_PIX  = 820
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = 
        WAVELNTH = 627.335
        GR_ORDER = 1
        CEN_PIX  = 990
        WAVEBAND = 2

DATAWIN
    DW_ID    = 611
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (75,62) pixels <14076>
    W_WIDTH  = 75
    W_HEIGHT = 62
    VDS_BACK = 1
    LL_ID    = 473
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_560_28                               
        WIN_DEF  = (380,421,75,62)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_30                             
        WIN_DEF  = (586,421,75,62)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_2_607_40                             
        WIN_DEF  = (783,421,75,62)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_627_34                               
        WIN_DEF  = (953,421,70,62)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 71
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(10,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 10
    NY       = 1

RASTER_VAR
    RAS_ID   = 71
    RAS_VAR  = 33
    RV_DESC  = (40x124) arcsec, 20s <QUIET>  Comp. 2 IDs-(473,611)
    EXPTIME  = 20
    LL_ID    = 473
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 611
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 247
    USABLE   = Y

STUDY
    STUDY_ID = 104
    TITLE_ID = 490
    OBS_PROG = BLINK_TE
    TITLE    = BLINKER STUDY (TEMPERATURE)
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 71
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 104
    TITLE_ID = 490
    STUDYVAR = 23
    SV_DESC  = TEMPERATURE VERSION (UPDATED LINE LIST) 4 WINDOWS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 247
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 71
        RAS_VAR  = 33
        N_REPEAT_R = 1
