DATATYPE = CDS STUDY DEFINITION
FILENAME = burst_1.def
INSTRUME = CDS
DATE_CRE = 1996/09/02 09:37:07
END

LINELIST
    LL_ID    = 104
    DETECTOR = N
    LL_DESC  = UV burst list - 7 windows, 25 pix
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.395
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne VI
        WAVELNTH = 562.949
        GR_ORDER = 1
        CEN_PIX  = 428
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O III
        WAVELNTH = 599.507
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O IV
        WAVELNTH = 617.083
        GR_ORDER = 1
        CEN_PIX  = 890
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Mg X
        WAVELNTH = 624
        GR_ORDER = 1
        CEN_PIX  = 949
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O IV
        WAVELNTH = 626.926
        GR_ORDER = 1
        CEN_PIX  = 974
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.8
        GR_ORDER = 1
        CEN_PIX  = 999
        WAVEBAND = 2

DATAWIN
    DW_ID    = 138
    DETECTOR = N
    DW_DESC  = Background,   7 lines.  dex = (25,16) pixels <12782>
    W_WIDTH  = 25
    W_HEIGHT = 16
    VDS_BACK = 1
    LL_ID    = 104
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = O_4_554_40                              
        WIN_DEF  = (343,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_6_562_95                             
        WIN_DEF  = (416,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_3_599_51                              
        WIN_DEF  = (728,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_4_617_08                              
        WIN_DEF  = (878,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_10_624_00                            
        WIN_DEF  = (937,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_4_626_93                              
        WIN_DEF  = (962,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_80                              
        WIN_DEF  = (987,444,25,16)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 96
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(8,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 8
    NY       = 1

RASTER_VAR
    RAS_ID   = 96
    RAS_VAR  = 1
    RV_DESC  = (32x32) arcsec, 5s <QUIET>  Comp. 2 IDs-(104,138)
    EXPTIME  = 5
    LL_ID    = 104
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 138
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 66
    USABLE   = Y

STUDY
    STUDY_ID = 134
    TITLE_ID = 228
    OBS_PROG = BURST
    TITLE    = TRANSITION REGION BURST STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 96
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 134
    TITLE_ID = 228
    STUDYVAR = 1
    SV_DESC  = VAR. 1, 32X32 ARCSEC, 4X240 SLIT
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 66
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 96
        RAS_VAR  = 1
        N_REPEAT_R = 20
