DATATYPE = CDS STUDY DEFINITION
FILENAME = cb_44_1.def
INSTRUME = CDS
DATE_CRE = 2004/09/23 16:10:34
END

LINELIST
    LL_ID    = 367
    DETECTOR = N
    LL_DESC  = AR new diagnostics
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 521.039
        GR_ORDER = 1
        CEN_PIX  = 81
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 368
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Si X
        WAVELNTH = 347.403
        GR_ORDER = 1
        CEN_PIX  = 574
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XIX
        WAVELNTH = 592.769
        GR_ORDER = 1
        CEN_PIX  = 695
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Si X
        WAVELNTH = 356.012
        GR_ORDER = 1
        CEN_PIX  = 697
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Mg X
        WAVELNTH = 625.627
        GR_ORDER = 1
        CEN_PIX  = 975
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.623
        GR_ORDER = 1
        CEN_PIX  = 1009
        WAVEBAND = 2

DATAWIN
    DW_ID    = 601
    DETECTOR = N
    DW_DESC  = Background,   7 lines. {367}  dex = (33,120) pixels <29457>
    W_WIDTH  = 33
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 367
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = Si_12_521_04                            
        WIN_DEF  = (65,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (352,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Si_10_347_40                            
        WIN_DEF  = (558,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_19_592_77                            
        WIN_DEF  = (679,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Si_10_356_01                            
        WIN_DEF  = (681,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_10_625_63                            
        WIN_DEF  = (959,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_62                              
        WIN_DEF  = (993,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 250
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(67,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 67
    NY       = 1

RASTER_VAR
    RAS_ID   = 250
    RAS_VAR  = 1
    RV_DESC  = (4x240) arcsec, 20s <ACTIVE>  Comp. (8,2) IDs-(367,601)
    EXPTIME  = 20
    LL_ID    = 367
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 601
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1781
    USABLE   = Y

STUDY
    STUDY_ID = 312
    TITLE_ID = 635
    OBS_PROG = CB_44
    TITLE    = OFF-LIMB AR DIAGNOSTICS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 250
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 312
    TITLE_ID = 635
    STUDYVAR = 1
    SV_DESC  = VARIATION 1, FT44 ORIGINAL LINE LIST
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1781
    ZONE_ID  = 1
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 250
        RAS_VAR  = 1
        N_REPEAT_R = 1
