DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/bmd2/CDS_STUDY/ch_so_wa_71.def
INSTRUME = CDS
DATE_CRE = 2003/03/31 14:22:00
END

LINELIST
    LL_ID    = 441
    DETECTOR = N
    LL_DESC  = QS-SO-Wavelength-Test
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = SiXII-HeI
        WAVELNTH = 523
        GR_ORDER = 1
        CEN_PIX  = 98
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = SiXI-HeI
        WAVELNTH = 582.6
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = OIV-MgX
        WAVELNTH = 609.1
        GR_ORDER = 1
        CEN_PIX  = 834
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = MgX-OV
        WAVELNTH = 627
        GR_ORDER = 1
        CEN_PIX  = 987
        WAVEBAND = 2

DATAWIN
    DW_ID    = 568
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (80,120) pixels <13864>
    W_WIDTH  = 80
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 441
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_523_00                               
        WIN_DEF  = (58,392,80,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_582_60                               
        WIN_DEF  = (568,392,80,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_609_10                               
        WIN_DEF  = (794,392,80,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_627_00                               
        WIN_DEF  = (947,392,76,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 78
    RV_DESC  = (240x240) arcsec, 100s <CORONA>  Comp. 2 IDs-(441,568)
    EXPTIME  = 100
    LL_ID    = 441
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 568
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 13000
    USABLE   = Y

STUDY
    STUDY_ID = 10
    TITLE_ID = 583
    OBS_PROG = CH_SO_WA
    TITLE    = CH/SOLAR-ORBITER/WAVELENGTH-TEST
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 10
    TITLE_ID = 583
    STUDYVAR = 71
    SV_DESC  = CH, 100 S, 4 WINDOWS, 2'X240'
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 13000
    ZONE_ID  = 3
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 78
        N_REPEAT_R = 1
