DATATYPE = CDS STUDY DEFINITION
FILENAME = chrom_n2_1.def
INSTRUME = CDS
DATE_CRE = 1996/05/10 09:50:04
END

LINELIST
    LL_ID    = 47
    DETECTOR = N
    LL_DESC  = O IV, Mg X lines
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = O IV lines
        WAVELNTH = 554.153
        GR_ORDER = 1
        CEN_PIX  = 350
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg X lines
        WAVELNTH = 608.211
        GR_ORDER = 1
        CEN_PIX  = 812
        WAVEBAND = 2

DATAWIN
    DW_ID    = 103
    DETECTOR = N
    DW_DESC  = Background,   2 lines.  dex = (45,90) pixels <6343>
    W_WIDTH  = 45
    W_HEIGHT = 90
    VDS_BACK = 1
    LL_ID    = 47
    N_WINS   = 6
    DW_IND   = 1
        WIN_NAME = O_4_554_15                              
        WIN_DEF  = (331,407,45,90)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_10_608_21                            
        WIN_DEF  = (792,407,45,90)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 48
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(2,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 2
    NY       = 1

RASTER_VAR
    RAS_ID   = 48
    RAS_VAR  = 2
    RV_DESC  = (8x180) arcsec, 10s <QUIET>  Comp. 2 IDs-(47,103)
    EXPTIME  = 10
    LL_ID    = 47
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 103
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 36
    USABLE   = Y

STUDY
    STUDY_ID = 107
    TITLE_ID = 179
    OBS_PROG = CHROM_N2
    TITLE    = CHROMOSPHERIC OSCILLATIONS 2
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 48
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 107
    TITLE_ID = 179
    STUDYVAR = 1
    SV_DESC  = 10 S, 2 LINES
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 36
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 48
        RAS_VAR  = 2
        N_REPEAT_R = 100
