DATATYPE = CDS STUDY DEFINITION
FILENAME = chrom_n4_8.def
INSTRUME = CDS
DATE_CRE = 1998/02/19 14:51:57
END

LINELIST
    LL_ID    = 234
    DETECTOR = N
    LL_DESC  = Chromospheric Oscillations - Hi-rate 2 lines
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = Fe XVI
        WAVELNTH = 335.425
        GR_ORDER = 1
        CEN_PIX  = 398
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1

DATAWIN
    DW_ID    = 312
    DETECTOR = N
    DW_DESC  = 2 lines. {0}  dex = (30,60) pixels <2494>
    W_WIDTH  = 30
    W_HEIGHT = 60
    VDS_BACK = 0
    LL_ID    = 234
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = Fe_16_335_42                            
        WIN_DEF  = (383,542,30,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (847,542,30,60)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 61
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(200,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 200
    NY       = 1

RASTER_VAR
    RAS_ID   = 61
    RAS_VAR  = 8
    RV_DESC  = (4x120) arcsec, 3s <QUIET>  Comp. 2 IDs-(234,312)
    EXPTIME  = 3
    LL_ID    = 234
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 312
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 1303
    USABLE   = Y

STUDY
    STUDY_ID = 74
    TITLE_ID = 132
    OBS_PROG = CHROM_N4
    TITLE    = CHROMOSPHERIC OSCILLATIONS: FOUR LINES
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 61
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 74
    TITLE_ID = 132
    STUDYVAR = 8
    SV_DESC  = 4X120 3 S, AR STUDY, MG IX 368, FE XVI 335 - HI-RATE
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1303
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 61
        RAS_VAR  = 8
        N_REPEAT_R = 1
