DATATYPE = CDS STUDY DEFINITION
FILENAME = fe15_op_2.def
INSTRUME = CDS
DATE_CRE = 2004/08/25 14:23:54
END

LINELIST
    LL_ID    = 466
    DETECTOR = N
    LL_DESC  = Revised to add FeXV
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.665
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XV
        WAVELNTH = 321.8
        GR_ORDER = 1
        CEN_PIX  = 209
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Fe XV
        WAVELNTH = 327.03
        GR_ORDER = 1
        CEN_PIX  = 284
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XIX
        WAVELNTH = 592.183
        GR_ORDER = 1
        CEN_PIX  = 690
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 764
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = O V
        WAVELNTH = 629.505
        GR_ORDER = 1
        CEN_PIX  = 1008
        WAVEBAND = 2

DATAWIN
    DW_ID    = 600
    DETECTOR = N
    DW_DESC  = Background,  10 lines. {0}  dex = (41,120) pixels <51941>
    W_WIDTH  = 41
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 466
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (58,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_15_321_80                            
        WIN_DEF  = (189,512,41,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_15_327_03                            
        WIN_DEF  = (264,512,41,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (603,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_19_592_18                            
        WIN_DEF  = (670,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (733,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (744,512,41,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (848,512,41,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (949,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = O_5_629_51                              
        WIN_DEF  = (988,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 11
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(60,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 11
    RAS_VAR  = 119
    RV_DESC  = (240x240) arcsec, 45s <ACTIVE>  Comp. (8,2) IDs-(466,600)
    EXPTIME  = 45
    LL_ID    = 466
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 600
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3250
    USABLE   = Y

DATAWIN
    DW_ID    = 1
    DETECTOR = G
    DW_DESC  = GIS Band1234  <20484>
    W_WIDTH  = 2048
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 0
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = BB_GIS_1                                
        WIN_DEF  = (0,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = BB_GIS_2                                
        WIN_DEF  = (2048,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = BB_GIS_3                                
        WIN_DEF  = (4096,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = BB_GIS_4                                
        WIN_DEF  = (6144,0,2048,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 20
    DETECTOR = G
    RAS_DESC = Slit(4x4),Posns(10,10)@(4,4) steps
    SLIT_NUM = 2
    XSTEP    = 4
    YSTEP    = 4
    NX       = 10
    NY       = 10

RASTER_VAR
    RAS_ID   = 20
    RAS_VAR  = 2
    RV_DESC  = (40x40) arcsec, 15s <QUIET>  Comp. 1 IDs-(0,1)
    EXPTIME  = 15
    LL_ID    = 0
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 1
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = M
    DURATION = 1691
    USABLE   = Y

STUDY
    STUDY_ID = 311
    TITLE_ID = 633
    OBS_PROG = FE15_OP
    TITLE    = FE XV OPACITY STUDY WITH GIS & NIS - new lines
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 11
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 20
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 311
    TITLE_ID = 633
    STUDYVAR = 2
    SV_DESC  = FEXV OPACITY, GIS+NIS, NEW LINE LIST
    N_RASTERS0 = 1
    DURATION0 = 3250
    DURATION1 = 1691
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 11
        RAS_VAR  = 119
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 20
        RAS_VAR  = 2
        N_REPEAT_R = 1
