DATATYPE = CDS STUDY DEFINITION
FILENAME = fe_line1_2.def
INSTRUME = CDS
DATE_CRE = 1996/03/20 13:47:17
END

DATAWIN
    DW_ID    = 82
    DETECTOR = G
    DW_DESC  = GIS Band12  <6146>
    W_WIDTH  = 2048
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 0
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = BB_GIS_1                                
        WIN_DEF  = (0,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = BB_GIS_2                                
        WIN_DEF  = (2048,0,2048,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 62
    DETECTOR = G
    RAS_DESC = Slit(4x4),Posns(4,4)@(4,4) steps
    SLIT_NUM = 2
    XSTEP    = 4
    YSTEP    = 4
    NX       = 4
    NY       = 4

RASTER_VAR
    RAS_ID   = 62
    RAS_VAR  = 2
    RV_DESC  = (16x16) arcsec, 15s <QUIET>  Comp. 1 IDs-(0,82)
    EXPTIME  = 15
    LL_ID    = 0
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 82
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = M
    DURATION = 265
    USABLE   = Y

STUDY
    STUDY_ID = 86
    TITLE_ID = 139
    OBS_PROG = FE-LINE1
    TITLE    = COMPARE THEOR/OBS FEIX-XVI EUV LINES - PHASE 2
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 62
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 86
    TITLE_ID = 139
    STUDYVAR = 2
    SV_DESC  = PHASE 2 - SMALL APERTURE (ACTIVE REGION)
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 265
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 62
        RAS_VAR  = 2
        N_REPEAT_R = 5
