DATATYPE = CDS STUDY DEFINITION
FILENAME = ffcal_2_1.def
INSTRUME = CDS
DATE_CRE = 1996/10/02 16:05:49
END

DATAWIN
    DW_ID    = 146
    DETECTOR = N
    DW_DESC  = Background, All NIS2 <5672>
    W_WIDTH  = 1024
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 0
    N_WINS   = 5
    DW_IND   = 1
        WIN_NAME = BB_NIS_2                                
        WIN_DEF  = (0,392,1024,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 102
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(20,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 102
    RAS_VAR  = 1
    RV_DESC  = (90x240) arcsec, 100s <QUIET>  Comp. 2 IDs-(0,146)
    EXPTIME  = 100
    LL_ID    = 0
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 146
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3578
    USABLE   = Y

STUDY
    STUDY_ID = 142
    TITLE_ID = 238
    OBS_PROG = FFCAL_2
    TITLE    = FULL SPECTRAL EXTRACTION FFCAL
    CATEGORY = C
    VAR_POINT = N
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 102
        POINTING = 0
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 142
    TITLE_ID = 238
    STUDYVAR = 1
    SV_DESC  = FFCAL NIS2 ONLY
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3578
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 102
        RAS_VAR  = 1
        N_REPEAT_R = 1
