DATATYPE = CDS STUDY DEFINITION
FILENAME = filaw_9.def
INSTRUME = CDS
DATE_CRE = 2003/06/03 13:00:48
END

LINELIST
    LL_ID    = 446
    DETECTOR = N
    LL_DESC  = Tritschler filament study
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = Ne VI
        WAVELNTH = 562.711
        GR_ORDER = 1
        CEN_PIX  = 438
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 821
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O V
        WAVELNTH = 629.27
        GR_ORDER = 1
        CEN_PIX  = 1006
        WAVEBAND = 2

DATAWIN
    DW_ID    = 577
    DETECTOR = N
    DW_DESC  = Background,   6 lines. {0}  dex = (35,120) pixels <25168>
    W_WIDTH  = 35
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 446
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = Ne_6_562_71                             
        WIN_DEF  = (421,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (606,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (736,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (804,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (952,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_27                              
        WIN_DEF  = (989,392,34,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 127
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(40,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 40
    NY       = 1

RASTER_VAR
    RAS_ID   = 127
    RAS_VAR  = 9
    RV_DESC  = (160x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(446,577)
    EXPTIME  = 30
    LL_ID    = 446
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 577
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1475
    USABLE   = Y

STUDY
    STUDY_ID = 157
    TITLE_ID = 589
    OBS_PROG = FILAW
    TITLE    = FILAMENT STUDY - TRITSCHLER
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 127
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 157
    TITLE_ID = 589
    STUDYVAR = 9
    SV_DESC  = FILAMENT  VERSION #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1475
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 127
        RAS_VAR  = 9
        N_REPEAT_R = 1
