DATATYPE = CDS STUDY DEFINITION
FILENAME = fillfacn_10.def
INSTRUME = CDS
DATE_CRE = 1996/05/10 09:50:32
END

LINELIST
    LL_ID    = 77
    DETECTOR = N
    LL_DESC  = Filling factor line list (NIS)
    N_LINES  = 14
    LL_IND   = 1
        LINENAME = New VDS line
        WAVELNTH = 318.628
        GR_ORDER = 1
        CEN_PIX  = 158
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Fe XV
        WAVELNTH = 321.78
        GR_ORDER = 1
        CEN_PIX  = 203
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Fe XV
        WAVELNTH = 327.02
        GR_ORDER = 1
        CEN_PIX  = 278
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = New VDS line
        WAVELNTH = 331.045
        GR_ORDER = 1
        CEN_PIX  = 335
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Fe XII
        WAVELNTH = 338.26
        GR_ORDER = 1
        CEN_PIX  = 438
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Si X
        WAVELNTH = 347.4
        GR_ORDER = 1
        CEN_PIX  = 568
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XIII
        WAVELNTH = 348.18
        GR_ORDER = 1
        CEN_PIX  = 579
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Fe XIV
        WAVELNTH = 353.83
        GR_ORDER = 1
        CEN_PIX  = 660
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si X
        WAVELNTH = 356.04
        GR_ORDER = 1
        CEN_PIX  = 691
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = Fe XIII
        WAVELNTH = 359.64
        GR_ORDER = 1
        CEN_PIX  = 743
        WAVEBAND = 1
    LL_IND   = 12
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 759
        WAVEBAND = 1
    LL_IND   = 13
        LINENAME = Fe XII
        WAVELNTH = 364.47
        GR_ORDER = 1
        CEN_PIX  = 811
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = New VDS line
        WAVELNTH = 370.541
        GR_ORDER = 1
        CEN_PIX  = 898
        WAVEBAND = 1

DATAWIN
    DW_ID    = 104
    DETECTOR = N
    DW_DESC  = Background,  14 lines.  dex = (24,120) pixels <20653>
    W_WIDTH  = 24
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 77
    N_WINS   = 18
    DW_IND   = 1
        WIN_NAME = WW_318_63                               
        WIN_DEF  = (146,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_15_321_78                            
        WIN_DEF  = (191,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_15_327_02                            
        WIN_DEF  = (266,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_331_05                               
        WIN_DEF  = (323,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (368,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Fe_12_338_26                            
        WIN_DEF  = (426,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Si_10_347_40                            
        WIN_DEF  = (556,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_13_348_18                            
        WIN_DEF  = (567,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Fe_14_353_83                            
        WIN_DEF  = (648,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_10_356_04                            
        WIN_DEF  = (679,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Fe_13_359_64                            
        WIN_DEF  = (731,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (747,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Fe_12_364_47                            
        WIN_DEF  = (799,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = WW_370_54                               
        WIN_DEF  = (886,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 3
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 3
    RAS_VAR  = 12
    RV_DESC  = (240x240) arcsec, 50s <ACTIVE>  Comp. 2 IDs-(77,104)
    EXPTIME  = 50
    LL_ID    = 77
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 104
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 6445
    USABLE   = Y

STUDY
    STUDY_ID = 3
    TITLE_ID = 180
    OBS_PROG = FILLFACN
    TITLE    = FILLING FACTOR (NIS)
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 3
    TITLE_ID = 180
    STUDYVAR = 10
    SV_DESC  = VAR #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 6445
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        RAS_VAR  = 12
        N_REPEAT_R = 1
