DATATYPE = CDS STUDY DEFINITION
FILENAME = g_spic_4_4.def
INSTRUME = CDS
DATE_CRE = 1997/07/29 08:54:46
END

LINELIST
    LL_ID    = 222
    DETECTOR = N
    LL_DESC  = Fast spicule list (Garching) V2
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = 
        WAVELNTH = 552.724
        GR_ORDER = 1
        CEN_PIX  = 340
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = 
        WAVELNTH = 555.876
        GR_ORDER = 1
        CEN_PIX  = 367
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 324
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {189}  dex = (29,35) pixels <8390>
    W_WIDTH  = 29
    W_HEIGHT = 35
    VDS_BACK = 1
    LL_ID    = 222
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_552_72                               
        WIN_DEF  = (326,435,29,35)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_555_88                               
        WIN_DEF  = (353,435,29,35)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (596,435,29,35)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (983,435,29,35)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 5
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(10,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 10
    NY       = 1

RASTER_VAR
    RAS_ID   = 5
    RAS_VAR  = 20
    RV_DESC  = (20x70) arcsec, 7s <QUIET>  Comp. 2 IDs-(222,324)
    EXPTIME  = 7
    LL_ID    = 222
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 324
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 105
    USABLE   = Y

LINELIST
    LL_ID    = 215
    DETECTOR = N
    LL_DESC  = Fast spicule list - 3 lines (Garching)
    N_LINES  = 3
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 313
    DETECTOR = N
    DW_DESC  = Background,   3 lines. {0}  dex = (55,30) pixels <7581>
    W_WIDTH  = 55
    W_HEIGHT = 30
    VDS_BACK = 1
    LL_ID    = 215
    N_WINS   = 7
    DW_IND   = 1
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (328,437,55,30)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (583,437,55,30)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (970,437,53,30)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 29
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(1,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 1
    NY       = 1

RASTER_VAR
    RAS_ID   = 29
    RAS_VAR  = 11
    RV_DESC  = (90x60) arcsec, 15s <QUIET>  Comp. 2 IDs-(215,313)
    EXPTIME  = 15
    LL_ID    = 215
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 313
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 54
    USABLE   = Y

STUDY
    STUDY_ID = 224
    TITLE_ID = 399
    OBS_PROG = G_SPIC_4
    TITLE    = GARCHING - 2 NARROW 1 WIDE SLIT
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 5
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 29
        POINTING = -1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 224
    TITLE_ID = 399
    STUDYVAR = 4
    SV_DESC  = VAR 4 - 2 NARROW SLIT, ONE WIDE (15 SECS)
    N_RASTERS0 = 2
    DURATION0 = 210
    DURATION1 = 54
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 5
        RAS_VAR  = 20
        N_REPEAT_R = 2
    RAS_IND   = 2
        RAS_ID   = 29
        RAS_VAR  = 11
        N_REPEAT_R = 1
