DATATYPE = CDS STUDY DEFINITION
FILENAME = glow_2a_1.def
INSTRUME = CDS
DATE_CRE = 1997/06/20 12:25:51
END

DATAWIN
    DW_ID    = 4
    DETECTOR = G
    DW_DESC  = GIS Band1234  <20484>
    W_WIDTH  = 2048
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 0
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = BB_GIS_1                                
        WIN_DEF  = (0,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = BB_GIS_2                                
        WIN_DEF  = (2048,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = BB_GIS_3                                
        WIN_DEF  = (4096,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = BB_GIS_4                                
        WIN_DEF  = (6144,0,2048,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 142
    DETECTOR = G
    RAS_DESC = Slit(4x4),Posns(1,40)@(0,4) steps
    SLIT_NUM = 2
    XSTEP    = 0
    YSTEP    = 4
    NX       = 1
    NY       = 40

RASTER_VAR
    RAS_ID   = 142
    RAS_VAR  = 1
    RV_DESC  = (4x160) arcsec, 95s <QUIET>  Comp. 1 IDs-(0,4)
    EXPTIME  = 95
    LL_ID    = 0
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 4
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = L
    DURATION = -3915
    USABLE   = Y

STUDY
    STUDY_ID = 221
    TITLE_ID = 383
    OBS_PROG = GLOW_2A
    TITLE    = GIS LOW MODE TELEMETRY ON DISK #1
    CATEGORY = S
    VAR_POINT = N
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 142
        POINTING = 0
        INS_X    = 0
        INS_Y    = 900

STUDY_VAR
    STUDY_ID = 221
    TITLE_ID = 383
    STUDYVAR = 1
    SV_DESC  = VAR #1 POLAR REGION
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3915
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 142
        RAS_VAR  = 1
        N_REPEAT_R = 25
