DATATYPE = CDS STUDY DEFINITION
FILENAME = hel_hi_1.def
INSTRUME = CDS
DATE_CRE = 1998/02/26 09:29:23
END

LINELIST
    LL_ID    = 240
    DETECTOR = N
    LL_DESC  = OXFORD HELIUM Hi-Rate Telemetry Line List
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 537.035
        GR_ORDER = 1
        CEN_PIX  = 206
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O IV
        WAVELNTH = 554.2
        GR_ORDER = 1
        CEN_PIX  = 353
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O IV
        WAVELNTH = 555.29
        GR_ORDER = 1
        CEN_PIX  = 362
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 611
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 741
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O IV/Mg X
        WAVELNTH = 609.054
        GR_ORDER = 1
        CEN_PIX  = 821
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 957
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 318
    DETECTOR = N
    DW_DESC  = Background,  10 lines. {0}  dex = (30,120) pixels <16248>
    W_WIDTH  = 30
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 240
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = He_1_537_03                             
        WIN_DEF  = (191,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_4_554_20                              
        WIN_DEF  = (338,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_4_555_29                              
        WIN_DEF  = (348,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (596,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (726,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (794,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = WW_609_05                               
        WIN_DEF  = (807,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (847,512,30,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (942,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (983,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 92
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(20,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 92
    RAS_VAR  = 3
    RV_DESC  = (40x240) arcsec, 25s <QUIET>  Comp. 2 IDs-(240,318)
    EXPTIME  = 25
    LL_ID    = 240
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 318
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 650
    USABLE   = Y

RASTER
    RAS_ID   = 154
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(200,-)@(0,-) steps
    SLIT_NUM = 4
    XSTEP    = 0
    YSTEP    = 0
    NX       = 200
    NY       = 1

RASTER_VAR
    RAS_ID   = 154
    RAS_VAR  = 1
    RV_DESC  = (2x240) arcsec, 25s <QUIET>  Comp. 2 IDs-(240,318)
    EXPTIME  = 25
    LL_ID    = 240
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 318
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 6471
    USABLE   = Y

STUDY
    STUDY_ID = 187
    TITLE_ID = 365
    OBS_PROG = HEL_HI
    TITLE    = OXFORD HELIUM STUDY -- HI-RATE TELEMETRY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 3
    RAS_IND   = 1
        RAS_ID   = 92
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 154
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 3
        RAS_ID   = 92
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 187
    TITLE_ID = 365
    STUDYVAR = 1
    SV_DESC  = HI-RATE VERSION #1
    N_RASTERS0 = 2
    DURATION0 = 7121
    DURATION1 = 650
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 3
    RAS_IND   = 1
        RAS_ID   = 92
        RAS_VAR  = 3
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 154
        RAS_VAR  = 1
        N_REPEAT_R = 1
    RAS_IND   = 3
        RAS_ID   = 92
        RAS_VAR  = 3
        N_REPEAT_R = 1
