DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/master/work/heli80w_4.def
INSTRUME = CDS
DATE_CRE = 2009/04/08 14:11:55
END

LINELIST
    LL_ID    = 500
    DETECTOR = N
    LL_DESC  = Helium list 7
    N_LINES  = 11
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 521.388
        GR_ORDER = 1
        CEN_PIX  = 84
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O III
        WAVELNTH = 525.465
        GR_ORDER = 1
        CEN_PIX  = 119
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 537.355
        GR_ORDER = 1
        CEN_PIX  = 221
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Ne IV
        WAVELNTH = 543.892
        GR_ORDER = 1
        CEN_PIX  = 277
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ne V
        WAVELNTH = 572.63
        GR_ORDER = 1
        CEN_PIX  = 523
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = He I
        WAVELNTH = 584.452
        GR_ORDER = 1
        CEN_PIX  = 624
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = He I
        WAVELNTH = 592.3
        GR_ORDER = 1
        CEN_PIX  = 691
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = He II
        WAVELNTH = 303.5
        GR_ORDER = 2
        CEN_PIX  = 816
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = Mg X
        WAVELNTH = 610.477
        GR_ORDER = 1
        CEN_PIX  = 846
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O V
        WAVELNTH = 628.918
        GR_ORDER = 1
        CEN_PIX  = 1003
        WAVEBAND = 2

DATAWIN
    DW_ID    = 644
    DETECTOR = N
    DW_DESC  = Background,  11 lines. {0}  dex = (41,120) pixels <55048>
    W_WIDTH  = 41
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 500
    N_WINS   = 15
    DW_IND   = 1
        WIN_NAME = He_1_521_39                             
        WIN_DEF  = (64,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_3_525_47                              
        WIN_DEF  = (99,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_537_35                             
        WIN_DEF  = (201,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_4_543_89                             
        WIN_DEF  = (257,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_5_572_63                             
        WIN_DEF  = (503,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_1_584_45                             
        WIN_DEF  = (604,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = He_1_592_30                             
        WIN_DEF  = (671,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (733,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = He_2_303_50                             
        WIN_DEF  = (796,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Mg_10_610_48                            
        WIN_DEF  = (826,392,41,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_5_628_92                              
        WIN_DEF  = (983,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 77
    DETECTOR = N
    RAS_DESC = Area(80x240),slit(4x240),Posns(20,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 77
    RAS_VAR  = 5
    RV_DESC  = (80x240) arcsec, 45s <QUIET>  Comp. (8,2) IDs-(500,644)
    EXPTIME  = 45
    LL_ID    = 500
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 644
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1065
    USABLE   = Y

STUDY
    STUDY_ID = 97
    TITLE_ID = 680
    OBS_PROG = HELI80W
    TITLE    = HELIUM 80''
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 77
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 97
    TITLE_ID = 680
    STUDYVAR = 4
    SV_DESC  = 45 S, SUM 2 BINS, 11 LINES, 41 PIX
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1065
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 77
        RAS_VAR  = 5
        N_REPEAT_R = 1
