DATATYPE = CDS STUDY DEFINITION
FILENAME = ical1_n_1.def
INSTRUME = CDS
DATE_CRE = 1996/02/23 15:48:17
END

LINELIST
    LL_ID    = 12
    DETECTOR = N
    LL_DESC  = Intercalibration Line Selection
    N_LINES  = 13
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 313.73
        GR_ORDER = 1
        CEN_PIX  = 114
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Mg VIII
        WAVELNTH = 315.02
        GR_ORDER = 1
        CEN_PIX  = 131
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg VIII
        WAVELNTH = 317.01
        GR_ORDER = 1
        CEN_PIX  = 159
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XIII
        WAVELNTH = 320.8
        GR_ORDER = 1
        CEN_PIX  = 211
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Fe XV
        WAVELNTH = 321.78
        GR_ORDER = 1
        CEN_PIX  = 225
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Fe XV
        WAVELNTH = 327.02
        GR_ORDER = 1
        CEN_PIX  = 297
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XVI
        WAVELNTH = 335.4
        GR_ORDER = 1
        CEN_PIX  = 413
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Si IX
        WAVELNTH = 345.13
        GR_ORDER = 1
        CEN_PIX  = 547
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si XII
        WAVELNTH = 520.67
        GR_ORDER = 1
        CEN_PIX  = 64
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = Mg X
        WAVELNTH = 609.79
        GR_ORDER = 1
        CEN_PIX  = 825
        WAVEBAND = 2
    LL_IND   = 13
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 955
        WAVEBAND = 2

DATAWIN
    DW_ID    = 15
    DETECTOR = N
    DW_DESC  = 13 lines.  dex = (15,120) pixels <12785>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 0
    LL_ID    = 12
    N_WINS   = 13
    DW_IND   = 1
        WIN_NAME = Mg_8_313_73                             
        WIN_DEF  = (107,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_8_315_02                             
        WIN_DEF  = (124,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_8_317_01                             
        WIN_DEF  = (152,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_13_320_80                            
        WIN_DEF  = (204,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_15_321_78                            
        WIN_DEF  = (218,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Fe_15_327_02                            
        WIN_DEF  = (290,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (389,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_16_335_40                            
        WIN_DEF  = (406,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Si_9_345_13                             
        WIN_DEF  = (540,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_12_520_67                            
        WIN_DEF  = (57,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (601,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (818,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (948,512,15,120)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 9
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(15,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 15
    NY       = 1

RASTER_VAR
    RAS_ID   = 9
    RAS_VAR  = 1
    RV_DESC  = (60x240) arcsec, 80s <QUIET>  Comp. 1 IDs-(12,15)
    EXPTIME  = 80
    LL_ID    = 12
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 15
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1274
    USABLE   = Y

STUDY
    STUDY_ID = 71
    TITLE_ID = 113
    OBS_PROG = ICAL1_N
    TITLE    = INTERCAL1 - NIS PART
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 9
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 71
    TITLE_ID = 113
    STUDYVAR = 1
    SV_DESC  = VERSION 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1274
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 9
        RAS_VAR  = 1
        N_REPEAT_R = 1
