DATATYPE = CDS STUDY DEFINITION
FILENAME = large_t_11.def
INSTRUME = CDS
DATE_CRE = 1996/05/15 14:57:33
END

LINELIST
    LL_ID    = 80
    DETECTOR = N
    LL_DESC  = Quick temperature coverage - 6 lines
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.415
        GR_ORDER = 1
        CEN_PIX  = 65
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ca X
        WAVELNTH = 557.559
        GR_ORDER = 1
        CEN_PIX  = 382
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O III
        WAVELNTH = 599.507
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Fe XVI
        WAVELNTH = 360.79
        GR_ORDER = 1
        CEN_PIX  = 759
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Mg X
        WAVELNTH = 624.817
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O V
        WAVELNTH = 629.621
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 109
    DETECTOR = N
    DW_DESC  = Background,   6 lines.  dex = (17,120) pixels <11281>
    W_WIDTH  = 17
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 80
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = Si_12_520_41                            
        WIN_DEF  = (57,392,17,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ca_10_557_56                            
        WIN_DEF  = (374,392,17,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_3_599_51                              
        WIN_DEF  = (732,392,17,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_16_360_79                            
        WIN_DEF  = (751,512,17,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_10_624_82                            
        WIN_DEF  = (948,392,17,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_62                              
        WIN_DEF  = (989,392,17,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 3
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 3
    RAS_VAR  = 13
    RV_DESC  = (240x240) arcsec, 15s <QUIET>  Comp. 2 IDs-(80,109)
    EXPTIME  = 15
    LL_ID    = 80
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 109
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 2158
    USABLE   = Y

STUDY
    STUDY_ID = 3
    TITLE_ID = 185
    OBS_PROG = LARGE_T
    TITLE    = QUICK TEMP COVERAGE OF LARGE REGION IN 6 LINES
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 3
    TITLE_ID = 185
    STUDYVAR = 11
    SV_DESC  = VARIATION 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 2158
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 3
        RAS_VAR  = 13
        N_REPEAT_R = 1
