DATATYPE = CDS STUDY DEFINITION
FILENAME = loops_1_1.def
INSTRUME = CDS
DATE_CRE = 1996/10/18 10:18:10
END

LINELIST
    LL_ID    = 116
    DETECTOR = N
    LL_DESC  = Fast Loop List
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 154
    DETECTOR = N
    DW_DESC  = Background,   4 lines.  dex = (17,60) pixels <9567>
    W_WIDTH  = 17
    W_HEIGHT = 60
    VDS_BACK = 1
    LL_ID    = 116
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (602,422,17,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (750,542,17,60)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (854,542,17,60)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (989,422,17,60)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 103
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(40,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 40
    NY       = 1

RASTER_VAR
    RAS_ID   = 103
    RAS_VAR  = 1
    RV_DESC  = (80x120) arcsec, 20s <QUIET>  Comp. 2 IDs-(116,154)
    EXPTIME  = 20
    LL_ID    = 116
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 154
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 948
    USABLE   = Y

STUDY
    STUDY_ID = 143
    TITLE_ID = 243
    OBS_PROG = LOOPS_1
    TITLE    = LOOP MOVIE
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 103
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 143
    TITLE_ID = 243
    STUDYVAR = 1
    SV_DESC  = VARIATION 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 948
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 103
        RAS_VAR  = 1
        N_REPEAT_R = 1
