DATATYPE = CDS STUDY DEFINITION
FILENAME = /user2/fludra/cds/mai/loops_5_1.def
INSTRUME = CDS
DATE_CRE = 2000/03/22 22:27:23
END

LINELIST
    LL_ID    = 288
    DETECTOR = N
    LL_DESC  = Loops_3 v.2
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = Ca X/Ne VI
        WAVELNTH = 558.3
        GR_ORDER = 1
        CEN_PIX  = 400
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.27
        GR_ORDER = 1
        CEN_PIX  = 1006
        WAVEBAND = 2

DATAWIN
    DW_ID    = 377
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (35,60) pixels <14427>
    W_WIDTH  = 35
    W_HEIGHT = 60
    VDS_BACK = 1
    LL_ID    = 288
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_558_30                               
        WIN_DEF  = (383,422,35,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (606,422,35,60)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (851,542,35,60)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_27                              
        WIN_DEF  = (989,422,34,60)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 161
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(120,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 161
    RAS_VAR  = 1
    RV_DESC  = (4x120) arcsec, 10s <ACTIVE>  Comp. 2 IDs-(288,377)
    EXPTIME  = 10
    LL_ID    = 288
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 377
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1770
    USABLE   = Y

STUDY
    STUDY_ID = 195
    TITLE_ID = 396
    OBS_PROG = LOOPS_5
    TITLE    = LOOP RAPID VARIATIONS 5
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 161
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 195
    TITLE_ID = 396
    STUDYVAR = 1
    SV_DESC  = 10 S, 35 PIX, 4X120''
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1770
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 161
        RAS_VAR  = 1
        N_REPEAT_R = 1
