DATATYPE = CDS STUDY DEFINITION
FILENAME = movie_hi_2.def
INSTRUME = CDS
DATE_CRE = 1997/10/06 09:05:24
END

LINELIST
    LL_ID    = 210
    DETECTOR = N
    LL_DESC  = Fast movie, 2 lines,  OV  + Mg IX
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 282
    DETECTOR = N
    DW_DESC  = 2 lines. {0}  dex = (45,75) pixels <3005>
    W_WIDTH  = 45
    W_HEIGHT = 75
    VDS_BACK = 0
    LL_ID    = 210
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (840,535,45,75)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (975,415,45,75)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 145
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(250,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 250
    NY       = 1

RASTER_VAR
    RAS_ID   = 145
    RAS_VAR  = 3
    RV_DESC  = (90x150) arcsec, 1s <QUIET>  Comp. 2 IDs-(210,282)
    EXPTIME  = 1
    LL_ID    = 210
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 282
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1327
    USABLE   = Y

STUDY
    STUDY_ID = 178
    TITLE_ID = 331
    OBS_PROG = MOVIE_HI
    TITLE    = FAST MOVIE FOR HI RATE TELEMETRY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 145
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 178
    TITLE_ID = 331
    STUDYVAR = 2
    SV_DESC  = VARN #2 - HI RATE MOVIE (2 LINES)
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1327
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 145
        RAS_VAR  = 3
        N_REPEAT_R = 1
