DATATYPE = CDS STUDY DEFINITION
FILENAME = mpenn_1_3.def
INSTRUME = CDS
DATE_CRE = 1998/05/21 13:48:30
END

LINELIST
    LL_ID    = 261
    DETECTOR = N
    LL_DESC  = M Penn - half list
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 356
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne VI
        WAVELNTH = 562.711
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 611
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 809
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XII
        WAVELNTH = 364.467
        GR_ORDER = 1
        CEN_PIX  = 811
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Mg X
        WAVELNTH = 609.793
        GR_ORDER = 1
        CEN_PIX  = 828
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 344
    DETECTOR = N
    DW_DESC  = Background,   7 lines. {0}  dex = (15,120) pixels <30035>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 261
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (349,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_6_562_71                             
        WIN_DEF  = (419,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (604,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (802,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_12_364_47                            
        WIN_DEF  = (804,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (821,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (991,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 135
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(25,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 25
    NY       = 1

RASTER_VAR
    RAS_ID   = 135
    RAS_VAR  = 6
    RV_DESC  = (100x240) arcsec, 6s <QUIET>  Comp. (8,2) IDs-(261,344)
    EXPTIME  = 6
    LL_ID    = 261
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 344
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 301
    USABLE   = Y

STUDY
    STUDY_ID = 166
    TITLE_ID = 348
    OBS_PROG = MPENN_1
    TITLE    = M PENN GI PROPOSAL, HI-RATE RASTER
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 135
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 166
    TITLE_ID = 348
    STUDYVAR = 3
    SV_DESC  = VERSION #2 MEDIUM TLM RATE
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 301
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 135
        RAS_VAR  = 6
        N_REPEAT_R = 1
