DATATYPE = CDS STUDY DEFINITION
FILENAME = nsgscan2_1.def
INSTRUME = CDS
DATE_CRE = 1997/03/06 14:26:40
END

DATAWIN
    DW_ID    = 4
    DETECTOR = G
    DW_DESC  = GIS Band1234  <20484>
    W_WIDTH  = 2048
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 0
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = BB_GIS_1                                
        WIN_DEF  = (0,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = BB_GIS_2                                
        WIN_DEF  = (2048,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = BB_GIS_3                                
        WIN_DEF  = (4096,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = BB_GIS_4                                
        WIN_DEF  = (6144,0,2048,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 128
    DETECTOR = G
    RAS_DESC = Slit(4x4),Posns(1,30)@(0,4) steps
    SLIT_NUM = 2
    XSTEP    = 0
    YSTEP    = 4
    NX       = 1
    NY       = 30

RASTER_VAR
    RAS_ID   = 128
    RAS_VAR  = 1
    RV_DESC  = (4x120) arcsec, 400s <QUIET>  Comp. 1 IDs-(0,4)
    EXPTIME  = 400
    LL_ID    = 0
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 4
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = M
    DURATION = 12048
    USABLE   = Y

STUDY
    STUDY_ID = 196
    TITLE_ID = 334
    OBS_PROG = NSGSCAN2
    TITLE    = N-S 4X120 ARCSEC SCAN WITH SLIT 4X4 ALL LINES GIS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 128
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 196
    TITLE_ID = 334
    STUDYVAR = 1
    SV_DESC  = VARIATION 1 400S FOR CORONAL HOLES
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 12048
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 128
        RAS_VAR  = 1
        N_REPEAT_R = 1
