DATATYPE = CDS STUDY DEFINITION
FILENAME = o_fflows_10.def
INSTRUME = CDS
DATE_CRE = 1996/08/15 10:37:25
END

LINELIST
    LL_ID    = 101
    DETECTOR = N
    LL_DESC  = JOP029 lines (8)
    N_LINES  = 8
    LL_IND   = 1
        LINENAME = O III
        WAVELNTH = 525.8
        GR_ORDER = 1
        CEN_PIX  = 111
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 537.03
        GR_ORDER = 1
        CEN_PIX  = 207
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Ne VI
        WAVELNTH = 562.83
        GR_ORDER = 1
        CEN_PIX  = 427
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 741
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 863
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 957
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 134
    DETECTOR = N
    DW_DESC  = Background,   8 lines.  dex = (21,120) pixels <13354>
    W_WIDTH  = 21
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 101
    N_WINS   = 12
    DW_IND   = 1
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (101,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_537_03                             
        WIN_DEF  = (197,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (417,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (600,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (731,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (853,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (947,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (988,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 2
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 2
    RAS_VAR  = 19
    RV_DESC  = (120x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(101,134)
    EXPTIME  = 30
    LL_ID    = 101
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 134
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 2084
    USABLE   = Y

STUDY
    STUDY_ID = 32
    TITLE_ID = 224
    OBS_PROG = O_FFLOWS
    TITLE    = FILAMENT FLOWS WITH SUMER AND CDS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 32
    TITLE_ID = 224
    STUDYVAR = 10
    SV_DESC  = VARIATION 15, 5 RASTERS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 2084
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        RAS_VAR  = 19
        N_REPEAT_R = 5
