DATATYPE = CDS STUDY DEFINITION
FILENAME = o_flows_12.def
INSTRUME = CDS
DATE_CRE = 1996/03/11 16:39:25
END

LINELIST
    LL_ID    = 52
    DETECTOR = N
    LL_DESC  = Flow distribution study (4 lines)
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 353
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 864
        WAVEBAND = 1

DATAWIN
    DW_ID    = 70
    DETECTOR = N
    DW_DESC  = 4 lines.  dex = (15,120) pixels <4541>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 0
    LL_ID    = 52
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (346,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (389,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (601,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (857,512,15,120)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 15
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(1,-)@(0,-) steps
    SLIT_NUM = 4
    XSTEP    = 0
    YSTEP    = 0
    NX       = 1
    NY       = 1

RASTER_VAR
    RAS_ID   = 15
    RAS_VAR  = 14
    RV_DESC  = (2x240) arcsec, 3s <QUIET>  Comp. 2 IDs-(52,70)
    EXPTIME  = 3
    LL_ID    = 52
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 70
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 13
    USABLE   = Y

STUDY
    STUDY_ID = 17
    TITLE_ID = 126
    OBS_PROG = O_FLOWS
    TITLE    = FLOW DISTRIBUTION STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 15
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 17
    TITLE_ID = 126
    STUDYVAR = 12
    SV_DESC  = VARIATION 10, 10 RASTERS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 13
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 15
        RAS_VAR  = 14
        N_REPEAT_R = 10
