DATATYPE = CDS STUDY DEFINITION
FILENAME = o_trlmf1_9.def
INSTRUME = CDS
DATE_CRE = 1996/08/05 10:04:45
END

LINELIST
    LL_ID    = 95
    DETECTOR = N
    LL_DESC  = JOP041 Phase 2 lines
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 522.2
        GR_ORDER = 1
        CEN_PIX  = 80
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O III
        WAVELNTH = 525.8
        GR_ORDER = 1
        CEN_PIX  = 111
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 741
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 863
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 127
    DETECTOR = N
    DW_DESC  = Background,   6 lines.  dex = (21,120) pixels <10797>
    W_WIDTH  = 21
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 95
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = He_1_522_20                             
        WIN_DEF  = (70,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (101,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (600,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (731,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (853,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (988,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 2
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 2
    RAS_VAR  = 18
    RV_DESC  = (120x240) arcsec, 20s <QUIET>  Comp. 2 IDs-(95,127)
    EXPTIME  = 20
    LL_ID    = 95
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 127
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1477
    USABLE   = Y

STUDY
    STUDY_ID = 32
    TITLE_ID = 217
    OBS_PROG = O_TRLMF1
    TITLE    = CONNECTION BETWEEN TRANSITION REGION LINES AND PHOTOSPHERIC MAGNETIC FIELD
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 32
    TITLE_ID = 217
    STUDYVAR = 9
    SV_DESC  = VARIATION 14, 3 RASTERS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1477
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        RAS_VAR  = 18
        N_REPEAT_R = 3
