DATATYPE = CDS STUDY DEFINITION
FILENAME = rah_fast_16.def
INSTRUME = CDS
DATE_CRE = 1996/12/02 16:30:54
END

LINELIST
    LL_ID    = 135
    DETECTOR = N
    LL_DESC  = NIS Bright Line List
    N_LINES  = 18
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.67
        GR_ORDER = 1
        CEN_PIX  = 67
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne IV
        WAVELNTH = 543.8
        GR_ORDER = 1
        CEN_PIX  = 264
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O IV
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 356
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Ca X
        WAVELNTH = 557.76
        GR_ORDER = 1
        CEN_PIX  = 383
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ne VI
        WAVELNTH = 562.83
        GR_ORDER = 1
        CEN_PIX  = 427
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Si IX
        WAVELNTH = 345.13
        GR_ORDER = 1
        CEN_PIX  = 536
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Si X
        WAVELNTH = 347.4
        GR_ORDER = 1
        CEN_PIX  = 569
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Si IX
        WAVELNTH = 349.87
        GR_ORDER = 1
        CEN_PIX  = 604
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = Si X
        WAVELNTH = 356.04
        GR_ORDER = 1
        CEN_PIX  = 691
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 759
        WAVEBAND = 1
    LL_IND   = 13
        LINENAME = He II
        WAVELNTH = 607.56
        GR_ORDER = 1
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 14
        LINENAME = Fe XII
        WAVELNTH = 364.47
        GR_ORDER = 1
        CEN_PIX  = 811
        WAVEBAND = 1
    LL_IND   = 15
        LINENAME = Mg X
        WAVELNTH = 609.79
        GR_ORDER = 1
        CEN_PIX  = 827
        WAVEBAND = 2
    LL_IND   = 16
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 863
        WAVEBAND = 1
    LL_IND   = 17
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 957
        WAVEBAND = 2
    LL_IND   = 18
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 183
    DETECTOR = N
    DW_DESC  = Background,  18 lines. {0}  dex = (22,60) pixels <25113>
    W_WIDTH  = 22
    W_HEIGHT = 60
    VDS_BACK = 1
    LL_ID    = 135
    N_WINS   = 22
    DW_IND   = 1
        WIN_NAME = Si_12_520_67                            
        WIN_DEF  = (54,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_4_543_80                             
        WIN_DEF  = (253,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (344,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ca_10_557_76                            
        WIN_DEF  = (372,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (416,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Si_9_345_13                             
        WIN_DEF  = (525,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Si_10_347_40                            
        WIN_DEF  = (558,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Si_9_349_87                             
        WIN_DEF  = (593,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (599,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_10_356_04                            
        WIN_DEF  = (680,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (729,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (747,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = He_2_607_56                             
        WIN_DEF  = (797,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Fe_12_364_47                            
        WIN_DEF  = (800,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (816,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (851,542,22,60)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (945,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (986,422,22,60)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 21
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 22
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 2
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 2
    RAS_VAR  = 26
    RV_DESC  = (120x120) arcsec, 15s <QUIET>  Comp. 2 IDs-(135,183)
    EXPTIME  = 15
    LL_ID    = 135
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 183
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1875
    USABLE   = Y

STUDY
    STUDY_ID = 32
    TITLE_ID = 267
    OBS_PROG = RAH_FAST
    TITLE    = FAST SURVEY RASTER
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 32
    TITLE_ID = 267
    STUDYVAR = 16
    SV_DESC  = VAR 1, FOR FAST TELEMETRY SUBMODE TEST
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1875
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 2
        RAS_VAR  = 26
        N_REPEAT_R = 1
