DATATYPE = CDS STUDY DEFINITION
FILENAME = /cs/data/plan/database/export/rgv_1.def
INSTRUME = CDS
DATE_CRE = 1997/03/05 13:32:01
END

LINELIST
    LL_ID    = 130
    DETECTOR = N
    LL_DESC  = K2LB
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 246
    DETECTOR = N
    DW_DESC  = 2 lines. {0}  dex = (45,50) pixels <2607>
    W_WIDTH  = 45
    W_HEIGHT = 50
    VDS_BACK = 0
    LL_ID    = 130
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (588,427,45,50)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (975,427,45,50)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 132
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(200,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 200
    NY       = 1

RASTER_VAR
    RAS_ID   = 132
    RAS_VAR  = 1
    RV_DESC  = (90x100) arcsec, 2s <QUIET>  Comp. 2 IDs-(130,246)
    EXPTIME  = 2
    LL_ID    = 130
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 246
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1370
    USABLE   = Y

STUDY
    STUDY_ID = 201
    TITLE_ID = 342
    OBS_PROG = RGV
    TITLE    = HIGH CADENCE TEST
    CATEGORY = T
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 132
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 201
    TITLE_ID = 342
    STUDYVAR = 1
    SV_DESC  = VERSION #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1370
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 132
        RAS_VAR  = 1
        N_REPEAT_R = 1
