DATATYPE = CDS STUDY DEFINITION
FILENAME = ser150w_2.def
INSTRUME = CDS
DATE_CRE = 2002/11/15 17:34:57
END

LINELIST
    LL_ID    = 393
    DETECTOR = N
    LL_DESC  = line width at limb
    N_LINES  = 11
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.665
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XIV
        WAVELNTH = 334.172
        GR_ORDER = 1
        CEN_PIX  = 386
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Si IX
        WAVELNTH = 341.949
        GR_ORDER = 1
        CEN_PIX  = 497
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XIII
        WAVELNTH = 348.183
        GR_ORDER = 1
        CEN_PIX  = 585
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Si IX
        WAVELNTH = 349.794
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Fe XIV
        WAVELNTH = 353.831
        GR_ORDER = 1
        CEN_PIX  = 666
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Fe XIII
        WAVELNTH = 359.842
        GR_ORDER = 1
        CEN_PIX  = 751
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Mg X
        WAVELNTH = 609.793
        GR_ORDER = 1
        CEN_PIX  = 840
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 1010
        WAVEBAND = 2

DATAWIN
    DW_ID    = 546
    DETECTOR = N
    DW_DESC  = Background,  11 lines. {0}  dex = (35,120) pixels <62172>
    W_WIDTH  = 35
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 393
    N_WINS   = 15
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (61,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (369,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Si_9_341_95                             
        WIN_DEF  = (480,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_13_348_18                            
        WIN_DEF  = (568,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Si_9_349_79                             
        WIN_DEF  = (591,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Fe_14_353_83                            
        WIN_DEF  = (649,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_13_359_84                            
        WIN_DEF  = (734,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (823,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (851,512,35,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (952,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (993,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 203
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(150,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 150
    NY       = 1

RASTER_VAR
    RAS_ID   = 203
    RAS_VAR  = 2
    RV_DESC  = (4x240) arcsec, 60s <QUIET>  Comp. 2 IDs-(393,546)
    EXPTIME  = 60
    LL_ID    = 393
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 546
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 10300
    USABLE   = Y

STUDY
    STUDY_ID = 257
    TITLE_ID = 559
    OBS_PROG = SER150W
    TITLE    = LINE WIDTHS AT LIMB
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 203
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 257
    TITLE_ID = 559
    STUDYVAR = 2
    SV_DESC  = VAR #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 10300
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 203
        RAS_VAR  = 2
        N_REPEAT_R = 1
