DATATYPE = CDS STUDY DEFINITION
FILENAME = sertscal_4.def
INSTRUME = CDS
DATE_CRE = 1996/10/02 15:57:45
END

LINELIST
    LL_ID    = 102
    DETECTOR = N
    LL_DESC  = SERTS Calibration Set
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 315.02
        GR_ORDER = 1
        CEN_PIX  = 107
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Si VIII
        WAVELNTH = 316.22
        GR_ORDER = 1
        CEN_PIX  = 124
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Si VIII
        WAVELNTH = 319.83
        GR_ORDER = 1
        CEN_PIX  = 175
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Fe XVI
        WAVELNTH = 335.4
        GR_ORDER = 1
        CEN_PIX  = 397
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Si X
        WAVELNTH = 347.4
        GR_ORDER = 1
        CEN_PIX  = 568
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Si IX
        WAVELNTH = 349.87
        GR_ORDER = 1
        CEN_PIX  = 603
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XII
        WAVELNTH = 352.11
        GR_ORDER = 1
        CEN_PIX  = 635
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Si X
        WAVELNTH = 356.04
        GR_ORDER = 1
        CEN_PIX  = 691
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 809
        WAVEBAND = 2

DATAWIN
    DW_ID    = 135
    DETECTOR = N
    DW_DESC  = Background,  10 lines.  dex = (15,120) pixels <14905>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 102
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = Mg_8_315_02                             
        WIN_DEF  = (100,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_8_316_22                             
        WIN_DEF  = (117,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Si_8_319_83                             
        WIN_DEF  = (168,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (373,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_16_335_40                            
        WIN_DEF  = (390,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Si_10_347_40                            
        WIN_DEF  = (561,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Si_9_349_87                             
        WIN_DEF  = (596,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_12_352_11                            
        WIN_DEF  = (628,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Si_10_356_04                            
        WIN_DEF  = (684,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (802,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 9
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(15,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 15
    NY       = 1

RASTER_VAR
    RAS_ID   = 9
    RAS_VAR  = 6
    RV_DESC  = (60x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(102,135)
    EXPTIME  = 30
    LL_ID    = 102
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 135
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 538
    USABLE   = Y

STUDY
    STUDY_ID = 71
    TITLE_ID = 226
    OBS_PROG = SERTSCAL
    TITLE    = SERTS CALIBRATION
    CATEGORY = C
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 9
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 71
    TITLE_ID = 226
    STUDYVAR = 4
    SV_DESC  = 10 LINE SET, 15 STEPS
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 538
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 9
        RAS_VAR  = 6
        N_REPEAT_R = 1
