DATATYPE = CDS STUDY DEFINITION
FILENAME = /tmp_mnt/disk7/thompson/usun/sertscl2_32.def
INSTRUME = CDS
DATE_CRE = 1997/11/06 21:29:03
END

LINELIST
    LL_ID    = 218
    DETECTOR = N
    LL_DESC  = SERTS intercalibration linelist #2, 16 lines
    N_LINES  = 16
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 314.854
        GR_ORDER = 1
        CEN_PIX  = 104
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Si VIII
        WAVELNTH = 316.391
        GR_ORDER = 1
        CEN_PIX  = 126
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Si VIII
        WAVELNTH = 319.83
        GR_ORDER = 1
        CEN_PIX  = 175
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XV
        WAVELNTH = 326.808
        GR_ORDER = 1
        CEN_PIX  = 275
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Cr XIII
        WAVELNTH = 328.348
        GR_ORDER = 1
        CEN_PIX  = 297
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Al X
        WAVELNTH = 332.551
        GR_ORDER = 1
        CEN_PIX  = 357
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Fe XIV
        WAVELNTH = 334.163
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XVI
        WAVELNTH = 335.776
        GR_ORDER = 1
        CEN_PIX  = 403
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg VIII
        WAVELNTH = 338.581
        GR_ORDER = 1
        CEN_PIX  = 443
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Si IX
        WAVELNTH = 341.529
        GR_ORDER = 1
        CEN_PIX  = 485
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = Si IX
        WAVELNTH = 345.13
        GR_ORDER = 1
        CEN_PIX  = 536
        WAVEBAND = 1
    LL_IND   = 12
        LINENAME = Si X
        WAVELNTH = 347.43
        GR_ORDER = 1
        CEN_PIX  = 569
        WAVEBAND = 1
    LL_IND   = 13
        LINENAME = Si IX
        WAVELNTH = 349.89
        GR_ORDER = 1
        CEN_PIX  = 604
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = Fe XII
        WAVELNTH = 352.352
        GR_ORDER = 1
        CEN_PIX  = 639
        WAVEBAND = 1
    LL_IND   = 15
        LINENAME = Fe XIV
        WAVELNTH = 353.901
        GR_ORDER = 1
        CEN_PIX  = 661
        WAVEBAND = 1
    LL_IND   = 16
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2

DATAWIN
    DW_ID    = 292
    DETECTOR = N
    DW_DESC  = Background,  16 lines. {0}  dex = (25,120) pixels <21198>
    W_WIDTH  = 25
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 218
    N_WINS   = 20
    DW_IND   = 1
        WIN_NAME = Mg_8_314_85                             
        WIN_DEF  = (92,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_8_316_39                             
        WIN_DEF  = (114,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Si_8_319_83                             
        WIN_DEF  = (163,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_15_326_81                            
        WIN_DEF  = (263,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Cr_13_328_35                            
        WIN_DEF  = (285,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Al_10_332_55                            
        WIN_DEF  = (345,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Fe_14_334_16                            
        WIN_DEF  = (368,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_16_335_78                            
        WIN_DEF  = (391,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_8_338_58                             
        WIN_DEF  = (431,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_9_341_53                             
        WIN_DEF  = (473,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Si_9_345_13                             
        WIN_DEF  = (524,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Si_10_347_43                            
        WIN_DEF  = (557,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Si_9_349_89                             
        WIN_DEF  = (592,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Fe_12_352_35                            
        WIN_DEF  = (627,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Fe_14_353_90                            
        WIN_DEF  = (649,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (796,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 38
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(30,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 38
    RAS_VAR  = 32
    RV_DESC  = (120x240) arcsec, 30s <QUIET>  Comp. 2 IDs-(218,292)
    EXPTIME  = 30
    LL_ID    = 218
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 292
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 1170
    USABLE   = Y

STUDY
    STUDY_ID = 44
    TITLE_ID = 342
    OBS_PROG = SERTSCL2
    TITLE    = SERTS CALIBRATION #2
    CATEGORY = C
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 44
    TITLE_ID = 342
    STUDYVAR = 32
    SV_DESC  = 16 LINE SET, 25 STEPS, LINE LIST #2A
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1170
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        RAS_VAR  = 32
        N_REPEAT_R = 1
