DATATYPE = CDS STUDY DEFINITION
FILENAME = sr_filb_6.def
INSTRUME = CDS
DATE_CRE = 2000/04/11 08:20:47
END

LINELIST
    LL_ID    = 334
    DETECTOR = N
    LL_DESC  = Regnier, filament, context
    N_LINES  = 3
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 584.92
        GR_ORDER = 1
        CEN_PIX  = 628
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O III
        WAVELNTH = 600.154
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He II
        WAVELNTH = 304.06
        GR_ORDER = 2
        CEN_PIX  = 826
        WAVEBAND = 2

DATAWIN
    DW_ID    = 471
    DETECTOR = N
    DW_DESC  = Background,   3 lines. {0}  dex = (43,120) pixels <10297>
    W_WIDTH  = 43
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 334
    N_WINS   = 7
    DW_IND   = 1
        WIN_NAME = He_1_584_92                             
        WIN_DEF  = (607,392,43,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_3_600_15                              
        WIN_DEF  = (737,392,43,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_2_304_06                             
        WIN_DEF  = (805,392,43,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 97
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(30,-)@(0,-) steps
    SLIT_NUM = 4
    XSTEP    = 0
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 97
    RAS_VAR  = 6
    RV_DESC  = (2x240) arcsec, 19s <QUIET>  Comp. 2 IDs-(334,471)
    EXPTIME  = 19
    LL_ID    = 334
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 471
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 730
    USABLE   = Y

STUDY
    STUDY_ID = 121
    TITLE_ID = 467
    OBS_PROG = SR_FILB
    TITLE    = REGNIER, FILAMENT, FIXED SLIT POSITION
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 97
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 121
    TITLE_ID = 467
    STUDYVAR = 6
    SV_DESC  = SR FILAMENT VAR #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 730
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 97
        RAS_VAR  = 6
        N_REPEAT_R = 1
