DATATYPE = CDS STUDY DEFINITION
FILENAME = sr_filc_56.def
INSTRUME = CDS
DATE_CRE = 2000/04/11 08:21:00
END

LINELIST
    LL_ID    = 335
    DETECTOR = N
    LL_DESC  = Regnier, filament, diagnostic
    N_LINES  = 10
    LL_IND   = 1
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 439
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Si IX
        WAVELNTH = 341.949
        GR_ORDER = 1
        CEN_PIX  = 497
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Ne V
        WAVELNTH = 572.098
        GR_ORDER = 1
        CEN_PIX  = 518
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Si XI
        WAVELNTH = 581.29
        GR_ORDER = 1
        CEN_PIX  = 597
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Si IX
        WAVELNTH = 349.794
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = He I
        WAVELNTH = 584.92
        GR_ORDER = 1
        CEN_PIX  = 628
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Ne V
        WAVELNTH = 359.382
        GR_ORDER = 1
        CEN_PIX  = 745
        WAVEBAND = 1
    LL_IND   = 8
        LINENAME = Fe XVI
        WAVELNTH = 361.178
        GR_ORDER = 1
        CEN_PIX  = 770
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Si XI
        WAVELNTH = 604.149
        GR_ORDER = 1
        CEN_PIX  = 792
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 1010
        WAVEBAND = 2

DATAWIN
    DW_ID    = 472
    DETECTOR = N
    DW_DESC  = Background,  10 lines. {0}  dex = (33,120) pixels <49968>
    W_WIDTH  = 33
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 335
    N_WINS   = 14
    DW_IND   = 1
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (423,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_9_341_95                             
        WIN_DEF  = (481,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Ne_5_572_10                             
        WIN_DEF  = (502,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Si_11_581_29                            
        WIN_DEF  = (581,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Si_9_349_79                             
        WIN_DEF  = (592,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_1_584_92                             
        WIN_DEF  = (612,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Ne_5_359_38                             
        WIN_DEF  = (729,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_16_361_18                            
        WIN_DEF  = (754,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Si_11_604_15                            
        WIN_DEF  = (776,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (994,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 68
    RV_DESC  = (240x240) arcsec, 40s <QUIET>  Comp. 2 IDs-(335,472)
    EXPTIME  = 40
    LL_ID    = 335
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 472
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 6610
    USABLE   = Y

STUDY
    STUDY_ID = 10
    TITLE_ID = 469
    OBS_PROG = SR_FILC
    TITLE    = REGNIER, FILAMENT, DIAGNOSTIC
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 10
    TITLE_ID = 469
    STUDYVAR = 56
    SV_DESC  = SR FILAMENT VAR #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 6610
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 68
        N_REPEAT_R = 1
