DATATYPE = CDS STUDY DEFINITION
FILENAME = /disk6/kucera/cds/ststr1_1.def
INSTRUME = CDS
DATE_CRE = 2002/01/09 22:14:12
END

LINELIST
    LL_ID    = 200
    DETECTOR = N
    LL_DESC  = EIT Wave I
    N_LINES  = 11
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.665
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O IV
        WAVELNTH = 553.3
        GR_ORDER = 1
        CEN_PIX  = 358
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Ca X/Ne VI/O
        WAVELNTH = 556
        GR_ORDER = 1
        CEN_PIX  = 381
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Ne VII
        WAVELNTH = 558.61
        GR_ORDER = 1
        CEN_PIX  = 403
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 439
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = Mg IX
        WAVELNTH = 368.068
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 272
    DETECTOR = N
    DW_DESC  = Background,  11 lines. {0}  dex = (25,120) pixels <59304>
    W_WIDTH  = 25
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 200
    N_WINS   = 15
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (66,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_4_553_30                              
        WIN_DEF  = (346,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_556_00                               
        WIN_DEF  = (369,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_7_558_61                             
        WIN_DEF  = (391,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (427,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (611,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (741,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (809,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (856,512,25,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (957,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (998,392,25,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 139
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(80,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 80
    NY       = 1

RASTER_VAR
    RAS_ID   = 139
    RAS_VAR  = 1
    RV_DESC  = (4x240) arcsec, 41s <QUIET>  Comp. 2 IDs-(200,272)
    EXPTIME  = 41
    LL_ID    = 200
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 272
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3832
    USABLE   = Y

STUDY
    STUDY_ID = 209
    TITLE_ID = 366
    OBS_PROG = STSTR1
    TITLE    = SIT AND STARE 1
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 139
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 209
    TITLE_ID = 366
    STUDYVAR = 1
    SV_DESC  = 41 SEC EXP,
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3832
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 139
        RAS_VAR  = 1
        N_REPEAT_R = 1

