DATATYPE = CDS STUDY DEFINITION
FILENAME = synop_lp_2.def
INSTRUME = CDS
DATE_CRE = 1997/12/12 13:57:02
END

LINELIST
    LL_ID    = 228
    DETECTOR = N
    LL_DESC  = LOW++ rate - OV only for synoptic
    N_LINES  = 1
    LL_IND   = 1
        LINENAME = O V 629.73
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 306
    DETECTOR = N
    DW_DESC  = Background,   1 lines. {227}  dex = (22,120) pixels <5656>
    W_WIDTH  = 22
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 228
    N_WINS   = 5
    DW_IND   = 1
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (986,392,22,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 49
    RV_DESC  = (240x240) arcsec, 15s <QUIET>  Comp. 2 IDs-(228,306)
    EXPTIME  = 15
    LL_ID    = 228
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 306
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = P
    DURATION = 2252
    USABLE   = Y

STUDY
    STUDY_ID = 37
    TITLE_ID = 352
    OBS_PROG = SYNOP_LP
    TITLE    = LOW++ RATE - SYNOPTIC
    CATEGORY = S
    VAR_POINT = N
    N_RASTER_DEF = 9
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 0
        INS_X    = 0
        INS_Y    = 880
    RAS_IND   = 2
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -220
    RAS_IND   = 3
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -440
    RAS_IND   = 4
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -660
    RAS_IND   = 5
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -880
    RAS_IND   = 6
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -1100
    RAS_IND   = 7
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -1320
    RAS_IND   = 8
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -1540
    RAS_IND   = 9
        RAS_ID   = 10
        POINTING = -1
        INS_X    = 0
        INS_Y    = -1760

STUDY_VAR
    STUDY_ID = 37
    TITLE_ID = 352
    STUDYVAR = 2
    SV_DESC  = SYNOPTIC, 9 RASTER VERSION LOW++ RATE, OV ONLY
    N_RASTERS0 = 8
    DURATION0 = 18016
    DURATION1 = 2252
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 9
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 3
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 4
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 5
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 6
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 7
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 8
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
    RAS_IND   = 9
        RAS_ID   = 10
        RAS_VAR  = 49
        N_REPEAT_R = 1
