DATATYPE = CDS STUDY DEFINITION
FILENAME = tdq33_1.def
INSTRUME = CDS
DATE_CRE = 1996/07/31 10:41:22
END

LINELIST
    LL_ID    = 91
    DETECTOR = N
    LL_DESC  = Active region temp & dens list - 7 lines, 20 pix
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = Fe XIV
        WAVELNTH = 333.922
        GR_ORDER = 1
        CEN_PIX  = 376
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = Fe XVI
        WAVELNTH = 335.325
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg V
        WAVELNTH = 353.424
        GR_ORDER = 1
        CEN_PIX  = 654
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XIV
        WAVELNTH = 354.827
        GR_ORDER = 1
        CEN_PIX  = 674
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Fe XIX
        WAVELNTH = 592.2
        GR_ORDER = 1
        CEN_PIX  = 678
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Mg X
        WAVELNTH = 624.817
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.621
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 122
    DETECTOR = N
    DW_DESC  = Background,   7 lines.  dex = (20,90) pixels <12896>
    W_WIDTH  = 20
    W_HEIGHT = 90
    VDS_BACK = 1
    LL_ID    = 91
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = Fe_14_333_92                            
        WIN_DEF  = (366,527,20,90)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_16_335_33                            
        WIN_DEF  = (386,527,20,90)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_5_353_42                             
        WIN_DEF  = (644,527,20,90)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_14_354_83                            
        WIN_DEF  = (664,527,20,90)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_19_592_20                            
        WIN_DEF  = (668,407,20,90)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_10_624_82                            
        WIN_DEF  = (946,407,20,90)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_62                              
        WIN_DEF  = (987,407,20,90)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 90
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(90,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 90
    NY       = 1

RASTER_VAR
    RAS_ID   = 90
    RAS_VAR  = 1
    RV_DESC  = (180x180) arcsec, 16s <QUIET>  Comp. 2 IDs-(91,122)
    EXPTIME  = 16
    LL_ID    = 91
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 122
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1860
    USABLE   = Y

STUDY
    STUDY_ID = 124
    TITLE_ID = 206
    OBS_PROG = TDQ33
    TITLE    = ACTIVE REGION TEMP & DENS STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 90
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 124
    TITLE_ID = 206
    STUDYVAR = 1
    SV_DESC  = VAR. 1, 3X3 RASTER, 2X240 SLIT
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1860
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 90
        RAS_VAR  = 1
        N_REPEAT_R = 1
