DATATYPE = CDS STUDY DEFINITION
FILENAME = tel_psf_7.def
INSTRUME = CDS
DATE_CRE = 2000/05/15 15:07:07
END

LINELIST
    LL_ID    = 341
    DETECTOR = N
    LL_DESC  = Mg PSF test
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = New VDS line
        WAVELNTH = 584.334
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = New VDS line
        WAVELNTH = 360.755
        GR_ORDER = 1
        CEN_PIX  = 764
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Mg X
        WAVELNTH = 625.3
        GR_ORDER = 1
        CEN_PIX  = 972
        WAVEBAND = 2

DATAWIN
    DW_ID    = 478
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (55,120) pixels <15017>
    W_WIDTH  = 55
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 341
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_584_33                               
        WIN_DEF  = (596,392,55,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_360_76                               
        WIN_DEF  = (737,512,55,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (841,512,55,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Mg_10_625_30                            
        WIN_DEF  = (945,392,55,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 133
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(40,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 40
    NY       = 1

RASTER_VAR
    RAS_ID   = 133
    RAS_VAR  = 8
    RV_DESC  = (90x240) arcsec, 35s <ACTIVE>  Comp. 2 IDs-(341,478)
    EXPTIME  = 35
    LL_ID    = 341
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 478
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1656
    USABLE   = Y

STUDY
    STUDY_ID = 164
    TITLE_ID = 475
    OBS_PROG = TEL_PSF
    TITLE    = NIS TEL PSF
    CATEGORY = T
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 133
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 164
    TITLE_ID = 475
    STUDYVAR = 7
    SV_DESC  = VARIATION # 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1656
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 133
        RAS_VAR  = 8
        N_REPEAT_R = 1
