DATATYPE = CDS STUDY DEFINITION
FILENAME = transb_1.def
INSTRUME = CDS
DATE_CRE = 1996/03/29 15:02:52
END

LINELIST
    LL_ID    = 68
    DETECTOR = N
    LL_DESC  = Mg X doublet
    N_LINES  = 2
    LL_IND   = 1
        LINENAME = Mg X
        WAVELNTH = 609.79
        GR_ORDER = 1
        CEN_PIX  = 825
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 955
        WAVEBAND = 2

DATAWIN
    DW_ID    = 89
    DETECTOR = N
    DW_DESC  = 2 lines.  dex = (20,60) pixels <2764>
    W_WIDTH  = 20
    W_HEIGHT = 60
    VDS_BACK = 0
    LL_ID    = 68
    N_WINS   = 2
    DW_IND   = 1
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (815,422,20,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (945,422,20,60)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 67
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(61,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 61
    NY       = 1

RASTER_VAR
    RAS_ID   = 67
    RAS_VAR  = 1
    RV_DESC  = (122x120) arcsec, 1s <ACTIVE>  Comp. 1 IDs-(68,89)
    EXPTIME  = 1
    LL_ID    = 68
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 89
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 198
    USABLE   = Y

STUDY
    STUDY_ID = 92
    TITLE_ID = 147
    OBS_PROG = TRANSB
    TITLE    = TRANSIENT BRIGHTENINGS STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 67
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 92
    TITLE_ID = 147
    STUDYVAR = 1
    SV_DESC  = VARIATION 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 198
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 67
        RAS_VAR  = 1
        N_REPEAT_R = 1
