DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/young/cds/new_studies/transcan_2.def
INSTRUME = CDS
DATE_CRE = 2006/01/20 17:04:03
END

LINELIST
    LL_ID    = 481
    DETECTOR = N
    LL_DESC  = Transient brightenings line list (D. Haigh)
    N_LINES  = 3
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 584.92
        GR_ORDER = 1
        CEN_PIX  = 628
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg IX
        WAVELNTH = 368.1
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = O V
        WAVELNTH = 629.976
        GR_ORDER = 1
        CEN_PIX  = 1012
        WAVEBAND = 2

DATAWIN
    DW_ID    = 618
    DETECTOR = N
    DW_DESC  = Background,   3 lines. {0}  dex = (24,105) pixels <11170>
    W_WIDTH  = 24
    W_HEIGHT = 105
    VDS_BACK = 1
    LL_ID    = 481
    N_WINS   = 7
    DW_IND   = 1
        WIN_NAME = He_1_584_92                             
        WIN_DEF  = (616,400,24,105)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_9_368_10                             
        WIN_DEF  = (856,520,24,105)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_5_629_98                              
        WIN_DEF  = (1000,400,23,105)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 206
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(6,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 6
    NY       = 1

RASTER_VAR
    RAS_ID   = 206
    RAS_VAR  = 2
    RV_DESC  = (24x210) arcsec, 5.4s <QUIET>  Comp. 2 IDs-(481,618)
    EXPTIME  = 5.4
    LL_ID    = 481
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 618
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 61
    USABLE   = Y

STUDY
    STUDY_ID = 255
    TITLE_ID = 656
    OBS_PROG = TRANSCAN
    TITLE    = TRANSIENT BRIGHTENING STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 206
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 255
    TITLE_ID = 656
    STUDYVAR = 2
    SV_DESC  = VAR.1, 24X210", 3 LINES, 5.4S, 4X240
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 61
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 206
        RAS_VAR  = 2
        N_REPEAT_R = 10
