DATATYPE = CDS STUDY DEFINITION
FILENAME = trvfevol_1.def
INSTRUME = CDS
DATE_CRE = 1996/07/03 14:07:44
END

LINELIST
    LL_ID    = 87
    DETECTOR = N
    LL_DESC  = Transition region, various temps
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.278
        GR_ORDER = 1
        CEN_PIX  = 354
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ne VI
        WAVELNTH = 562.83
        GR_ORDER = 1
        CEN_PIX  = 427
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 741
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 117
    DETECTOR = N
    DW_DESC  = Background,   4 lines.  dex = (40,120) pixels <8784>
    W_WIDTH  = 40
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 87
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = O_4_554_28                               
        WIN_DEF  = (334,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (407,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (721,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (978,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 2
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 2
    RAS_VAR  = 17
    RV_DESC  = (120x240) arcsec, 25s <QUIET>  Comp. 2 IDs-(87,117)
    EXPTIME  = 25
    LL_ID    = 87
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 117
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1783
    USABLE   = Y

STUDY
    STUDY_ID = 117
    TITLE_ID = 196
    OBS_PROG = TRVFEVOL
    TITLE    = TR VELOCITY FIELD EVOLUTION
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 2
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 2
        POINTING = -1
        INS_X    = 5
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 117
    TITLE_ID = 196
    STUDYVAR = 1
    SV_DESC  = 2 RASTERS, HOUR LONG BLOCK
    N_RASTERS0 = 1
    DURATION0 = 1783
    DURATION1 = 1783
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 2
        RAS_VAR  = 17
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 2
        RAS_VAR  = 17
        N_REPEAT_R = 1
