DATATYPE = CDS STUDY DEFINITION
FILENAME = uly_quad_2.def
INSTRUME = CDS
DATE_CRE = 2003/10/23 11:06:49
END

LINELIST
    LL_ID    = 449
    DETECTOR = N
    LL_DESC  = Ulysses quadrature
    N_LINES  = 5
    LL_IND   = 1
        LINENAME = Si XI
        WAVELNTH = 580.908
        GR_ORDER = 1
        CEN_PIX  = 594
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Fe XIX
        WAVELNTH = 592.162
        GR_ORDER = 1
        CEN_PIX  = 690
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 764
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 1010
        WAVEBAND = 2

DATAWIN
    DW_ID    = 580
    DETECTOR = N
    DW_DESC  = Background,   5 lines. {0}  dex = (33,120) pixels <18753>
    W_WIDTH  = 33
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 449
    N_WINS   = 9
    DW_IND   = 1
        WIN_NAME = Si_11_580_91                            
        WIN_DEF  = (578,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (607,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_19_592_16                            
        WIN_DEF  = (674,392,33,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (748,512,33,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (994,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 199
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(25,-)@(6,-) steps
    SLIT_NUM = 5
    XSTEP    = 6
    YSTEP    = 0
    NX       = 25
    NY       = 1

RASTER_VAR
    RAS_ID   = 199
    RAS_VAR  = 2
    RV_DESC  = (148x240) arcsec, 12s <QUIET>  Comp. (8,2) IDs-(449,580)
    EXPTIME  = 12
    LL_ID    = 449
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 580
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 461
    USABLE   = Y

STUDY
    STUDY_ID = 246
    TITLE_ID = 596
    OBS_PROG = ULY_QUAD
    TITLE    = ULYSSES QUADRATURE
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 199
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 246
    TITLE_ID = 596
    STUDYVAR = 2
    SV_DESC  = VARN #1 ULY QUAD
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 461
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 199
        RAS_VAR  = 2
        N_REPEAT_R = 1
