LASCO/EIT Operations Status
Daily Reports --  Current Status
-----------------------------
Bogart synoptic = EIT synops every 12 hours at 01:00 and 13:00 UT
		  C2 at 12 minute cadence beginning at :00 minutes
		  C2 at 12 minute cadence beginning at :06 minutes
		  C2-C3 orange/blue filters daily 

Weekly, Dark Cal Images (Fri) C1,C2,C3 at 0 and 60 Sec, EIT at 0 and 3 sec. 
(Fri) C2,C3 SeqPW Deep Red Polarizer Sequence 
(Fri) C2,C3 SeqPw Color Sequence Images, 2x2 binned (03:00 UT)
-------------------------------------------------------------------------------
31-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

30-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

29-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

	14:10 UT uplinked l_set_lobt (set Lasco time)

28-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]	

27-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]
	
26-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180] 

25-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.
	
	15:34 UT uplinked l_set_lobt (set Lasco time)
	
24-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

23-August-2017  (Bogart synoptics) TM Submode 6; [S/C-180]

22-August-2017  (Bogart synoptics) TM Submode 5; [S/C-180]

	Orbit Keyhole #59 

	23:07 UT Transition TM Submode 5 -> 6

21-August-2017  (Bogart synoptics) TM Submode 5; [S/C-0]

20-August-2017  (Bogart synoptics) TM Submode 5; [S/C-0]

		14:25 UT uplinked l_set_lobt (set Lasco time)

19-August-2017  (Bogart synoptics) TM Submode 5; [S/C-0] 

18-August-2017  (Bogart synoptics) TM Submode 5; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

17-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Sector Hang
		
	01:00 UT EIT begins observation in 284A
	02:08 UT EIT temp @ 19.82C (standard monitor trigger point) - LEB reset.

	14:36 UT uplinked l_set_lobt (set Lasco time)
	14:29-15:07 UT LEB REBOOT
	15:48 UT Observation program resumed.
		12:45 hrs data gap (02:08 - 14:53 UT)

	Transition TM Submode 6 -> 5

	22:43 UT uplinked l_set_lobt (set Lasco time)

	00:01 UT take_sequence uploaded

16-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

15-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

	15:52 UT uplinked l_set_lobt (set Lasco time)

14-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
13-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

12-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

11-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:53  UT uplinked l_set_lobt (set Lasco time)

10-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

09-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
		                                                                                                  
08-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:52 UT uplinked l_set_lobt (set Lasco time)
	
07-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

06-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

05-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
04-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:51 UT uplinked l_set_lobt (set Lasco time)

03-August-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	       
02-August-2017  (Bogart synoptics) TM submode 6; [S/C-0]
	
01-August-2017  (Bogart synoptics) TM submode 6; [S/C-0]