LASCO/EIT Operations Status
Daily Reports --  Current Status
-----------------------------
Bogart synoptic = EIT synops every 12 hours at 01:00 and 13:00 UT
		  C2 at 12 minute cadence beginning at :00 minutes
		  C2 at 12 minute cadence beginning at :06 minutes
		  C2-C3 orange/blue filters daily 

Weekly, Dark Cal Images (Fri) C1,C2,C3 at 0 and 60 Sec, EIT at 0 and 3 sec. 
(Fri) C2,C3 SeqPW Deep Red Polarizer Sequence 
(Fri) C2,C3 SeqPw Color Sequence Images, 2x2 binned (03:00 UT)
-------------------------------------------------------------------------------
31-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:35 UT uplinked l_set_lobt (set Lasco time)

30-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
29-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

28-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:36 UT uplinked l_set_lobt (set Lasco time)

27-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
26-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

25-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
24-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:33 UT uplinked l_set_lobt (set Lasco time)
	
23-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

22-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

21-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:35 UT uplinked l_set_lobt (set Lasco time)
	
20-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

19-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

18-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
17-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:35 UT uplinked l_set_lobt (set Lasco time)

16-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

15-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

14-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.
	
13-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

12-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

11-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

	13:54 UT uplinked l_set_lobt (set Lasco time)	

10-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

09-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
		                                                                                                  
08-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
07-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
           Weekly EIT calibration lamps x2 taken.
           Weekly C2,C3 SeqPW color sequence taken.
           Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.
	
	12:57 UT uplinked l_set_lobt (set Lasco time)

06-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

05-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
04-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

03-July-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:39 UT uplinked l_set_lobt (set Lasco time)
	       
02-July-2017  (Bogart synoptics) TM submode 6; [S/C-0]
	
01-July-2017  (Bogart synoptics) TM submode 6; [S/C-0]