LASCO/EIT Operations Status
Daily Reports --  Current Status
-----------------------------
Bogart synoptic = EIT synops every 12 hours at 01:00 and 13:00 UT
		  C2 at 12 minute cadence beginning at :00 minutes
		  C2 at 12 minute cadence beginning at :06 minutes
		  C2-C3 orange/blue filters daily 

Weekly, Dark Cal Images (Fri) C1,C2,C3 at 0 and 60 Sec, EIT at 0 and 3 sec. 
(Fri) C2,C3 SeqPW Deep Red Polarizer Sequence 
(Fri) C2,C3 SeqPw Color Sequence Images, 2x2 binned (03:00 UT)
-------------------------------------------------------------------------------
30-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
        Weekly EIT calibration lamps x2 taken.
        Weekly C2,C3 SeqPW color sequence taken.
        Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:36 UT uplinked l_set_lobt (set Lasco time)
	
29-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

28-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

27-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	12:26 UT uplinked l_set_lobt (set Lasco time)
	
26-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

25-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
24-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
23-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
        Weekly EIT calibration lamps x2 taken.
        Weekly C2,C3 SeqPW color sequence taken.
        Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	13:33 UT uplinked l_set_lobt (set Lasco time)

22-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

21-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
20-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

19-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 

	13:31 UT uplinked l_set_lobt (set Lasco time)

18-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
17-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

16-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
        Weekly EIT calibration lamps x2 taken.
        Weekly C2,C3 SeqPW color sequence taken.
        Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

15-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	13:06 UT uplinked l_set_lobt (set Lasco time)

14-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
13-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

12-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

11-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0] 	

10-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Annual Calibration Sets end: 10:09 UT

09-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

	Weekly C2,C3,EIT dark images taken.
        Weekly EIT calibration lamps x2 taken.
        Weekly C2,C3 SeqPW color sequence taken.
        Weekly C2,C3 SeqPW deep red filter polarizer sequence taken.

	Annual Calibration Sets begin: 12:27 UT
	12:29 UT uplinked l_set_lobt (set Lasco time)
	                                                                                                  
08-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
07-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

06-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

05-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	
04-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]

03-June-2017  (Bogart synoptics) TM Submode 6; [S/C-0]
	       
02-June-2017  (Bogart synoptics) TM submode 6; [S/C-0]

	14:24-16:54 UT LEB REBOOT
	02:30 hrs data gap (14:24-16:54UT)
	
01-June-2017  (Bogart synoptics) TM submode 6; [S/C-0]

	13:56 UT uplinked l_set_lobt (set Lasco time)

	14:19-15:24 UT LEB REBOOT
	01:05 hrs data gap (14:19 - 15:24 UT)