DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/eoshea/arem_24_95.def
INSTRUME = CDS
DATE_CRE = 2001/07/03 09:52:05
END

LINELIST
    LL_ID    = 400
    DETECTOR = N
    LL_DESC  = New Dem lines
    N_LINES  = 20
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 521.3
        GR_ORDER = 1
        CEN_PIX  = 83
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg VIII
        WAVELNTH = 315.013
        GR_ORDER = 1
        CEN_PIX  = 112
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg VIII
        WAVELNTH = 317.597
        GR_ORDER = 1
        CEN_PIX  = 149
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Ne IV
        WAVELNTH = 543.892
        GR_ORDER = 1
        CEN_PIX  = 277
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Al XI
        WAVELNTH = 549.75
        GR_ORDER = 1
        CEN_PIX  = 327
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O IV
        WAVELNTH = 554.1
        GR_ORDER = 1
        CEN_PIX  = 364
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Ca X
        WAVELNTH = 558.4
        GR_ORDER = 1
        CEN_PIX  = 401
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Ne VI
        WAVELNTH = 562.7
        GR_ORDER = 1
        CEN_PIX  = 438
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = Ne V
        WAVELNTH = 572.331
        GR_ORDER = 1
        CEN_PIX  = 520
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = Si IX
        WAVELNTH = 344.4
        GR_ORDER = 1
        CEN_PIX  = 532
        WAVEBAND = 1
    LL_IND   = 11
        LINENAME = Si X
        WAVELNTH = 347.003
        GR_ORDER = 1
        CEN_PIX  = 569
        WAVEBAND = 1
    LL_IND   = 12
        LINENAME = Si XI
        WAVELNTH = 580.908
        GR_ORDER = 1
        CEN_PIX  = 594
        WAVEBAND = 2
    LL_IND   = 13
        LINENAME = Mg VI
        WAVELNTH = 349.65
        GR_ORDER = 1
        CEN_PIX  = 606
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 15
        LINENAME = Si X
        WAVELNTH = 356.212
        GR_ORDER = 1
        CEN_PIX  = 700
        WAVEBAND = 1
    LL_IND   = 16
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 17
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 764
        WAVEBAND = 1
    LL_IND   = 18
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 19
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 20
        LINENAME = O V
        WAVELNTH = 629.505
        GR_ORDER = 1
        CEN_PIX  = 1008
        WAVEBAND = 2

DATAWIN
    DW_ID    = 519
    DETECTOR = N
    DW_DESC  = Background,  20 lines. {400}  dex = (40,120) pixels <153641>
    W_WIDTH  = 40
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 400
    N_WINS   = 24
    DW_IND   = 1
        WIN_NAME = Si_12_521_30                            
        WIN_DEF  = (63,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_8_315_01                             
        WIN_DEF  = (92,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_8_317_60                             
        WIN_DEF  = (129,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_4_543_89                             
        WIN_DEF  = (257,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Al_11_549_75                            
        WIN_DEF  = (307,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_4_554_10                              
        WIN_DEF  = (344,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Ca_10_558_40                            
        WIN_DEF  = (381,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Ne_6_562_70                             
        WIN_DEF  = (418,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Ne_5_572_33                             
        WIN_DEF  = (500,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Si_9_344_40                             
        WIN_DEF  = (512,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Si_10_347_00                            
        WIN_DEF  = (549,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Si_11_580_91                            
        WIN_DEF  = (574,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Mg_6_349_65                             
        WIN_DEF  = (586,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (603,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Si_10_356_21                            
        WIN_DEF  = (680,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (733,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (744,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (848,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (949,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 20
        WIN_NAME = O_5_629_51                              
        WIN_DEF  = (988,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 21
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 22
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 23
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 24
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 11
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(60,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 11
    RAS_VAR  = 103
    RV_DESC  = (240x240) arcsec, 35s <ACTIVE>  Comp. (8,2) IDs-(400,519)
    EXPTIME  = 35
    LL_ID    = 400
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 519
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 5450
    USABLE   = Y

STUDY
    STUDY_ID = 11
    TITLE_ID = 520
    OBS_PROG = AREM_24
    TITLE    = AR_STRUCT_240
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 11
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 11
    TITLE_ID = 520
    STUDYVAR = 95
    SV_DESC  = 35 S, 240'' X 240'' FOV
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 5450
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 11
        RAS_VAR  = 103
        N_REPEAT_R = 1
