DATATYPE = CDS STUDY DEFINITION
FILENAME = chrom_n8_1.def
INSTRUME = CDS
DATE_CRE = 2001/08/23 07:45:17
END

LINELIST
    LL_ID    = 377
    DETECTOR = N
    LL_DESC  = Polar coronal hole study list
    N_LINES  = 11
    LL_IND   = 1
        LINENAME = Mg VIII
        WAVELNTH = 313.754
        GR_ORDER = 1
        CEN_PIX  = 94
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = O IV
        WAVELNTH = 554.513
        GR_ORDER = 1
        CEN_PIX  = 368
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Fe XIV
        WAVELNTH = 333.763
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XVI
        WAVELNTH = 335.726
        GR_ORDER = 1
        CEN_PIX  = 408
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Si X
        WAVELNTH = 356.05
        GR_ORDER = 1
        CEN_PIX  = 697
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Fe XII
        WAVELNTH = 364.467
        GR_ORDER = 1
        CEN_PIX  = 817
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O V
        WAVELNTH = 629.505
        GR_ORDER = 1
        CEN_PIX  = 1008
        WAVEBAND = 2

DATAWIN
    DW_ID    = 522
    DETECTOR = N
    DW_DESC  = Background,  11 lines. {0}  dex = (40,120) pixels <60899>
    W_WIDTH  = 40
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 377
    N_WINS   = 15
    DW_IND   = 1
        WIN_NAME = Mg_8_313_75                             
        WIN_DEF  = (74,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = O_4_554_51                              
        WIN_DEF  = (348,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_14_333_76                            
        WIN_DEF  = (360,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_16_335_73                            
        WIN_DEF  = (388,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (603,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Si_10_356_05                            
        WIN_DEF  = (677,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (733,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Fe_12_364_47                            
        WIN_DEF  = (797,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (848,512,40,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (949,392,40,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_5_629_51                              
        WIN_DEF  = (988,392,35,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 203
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(150,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 150
    NY       = 1

RASTER_VAR
    RAS_ID   = 203
    RAS_VAR  = 1
    RV_DESC  = (4x240) arcsec, 60s <QUIET>  Comp. 2 IDs-(377,522)
    EXPTIME  = 60
    LL_ID    = 377
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 522
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 11111
    USABLE   = Y

STUDY
    STUDY_ID = 257
    TITLE_ID = 523
    OBS_PROG = CHROM_N8
    TITLE    = POLAR CORONAL HOLE STUDY - BANERJEE
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 203
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 257
    TITLE_ID = 523
    STUDYVAR = 1
    SV_DESC  = VARIATION #1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 11111
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 203
        RAS_VAR  = 1
        N_REPEAT_R = 1
