DATATYPE = CDS STUDY DEFINITION
FILENAME = /home/master/jar/flaredop_4.def
INSTRUME = CDS
DATE_CRE = 2009/01/30 11:52:41
END

LINELIST
    LL_ID    = 459
    DETECTOR = N
    LL_DESC  = FLAREDOP linelist
    N_LINES  = 5
    LL_IND   = 1
        LINENAME = Si XII
        WAVELNTH = 520.665
        GR_ORDER = 1
        CEN_PIX  = 78
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 585
        GR_ORDER = 1
        CEN_PIX  = 629
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Window1
        WAVELNTH = 595.113
        GR_ORDER = 1
        CEN_PIX  = 715
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Window2
        WAVELNTH = 605.432
        GR_ORDER = 1
        CEN_PIX  = 803
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Window4
        WAVELNTH = 628
        GR_ORDER = 1
        CEN_PIX  = 995
        WAVEBAND = 2

DATAWIN
    DW_ID    = 637
    DETECTOR = N
    DW_DESC  = Background,   5 lines. {459}  dex = (89,60) pixels <17982>
    W_WIDTH  = 89
    W_HEIGHT = 60
    VDS_BACK = 1
    LL_ID    = 459
    N_WINS   = 9
    DW_IND   = 1
        WIN_NAME = Si_12_520_66                            
        WIN_DEF  = (34,422,89,60)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_585_00                             
        WIN_DEF  = (585,422,89,60)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_595_11                               
        WIN_DEF  = (671,422,89,60)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_605_43                               
        WIN_DEF  = (759,422,89,60)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = WW_628_00                               
        WIN_DEF  = (951,422,72,60)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 136
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(70,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 70
    NY       = 1

RASTER_VAR
    RAS_ID   = 136
    RAS_VAR  = 4
    RV_DESC  = (4x120) arcsec, 1.5s <ACTIVE>  Comp. (8,12) IDs-(459,637)
    EXPTIME  = 1.5
    LL_ID    = 459
    COMP_ID  = 8
    COMP_OPT = 12
    DW_ID    = 637
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 464
    USABLE   = Y

STUDY
    STUDY_ID = 167
    TITLE_ID = 618
    OBS_PROG = FLAREDOP
    TITLE    = FLARE DOPPLER SHIFTS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 136
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 167
    TITLE_ID = 618
    STUDYVAR = 4
    SV_DESC  = 4X240 SLIT, 1.5 S, COMPRESS BY 12, 70 REPEATS, HEIGHT=120
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 464
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 136
        RAS_VAR  = 4
        N_REPEAT_R = 1
