DATATYPE = CDS STUDY DEFINITION
FILENAME = g_spic_1_17.def
INSTRUME = CDS
DATE_CRE = 1997/06/26 15:38:21
END

LINELIST
    LL_ID    = 214
    DETECTOR = N
    LL_DESC  = Fast spicule list (Garching)
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = 
        WAVELNTH = 552.724
        GR_ORDER = 1
        CEN_PIX  = 340
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = 
        WAVELNTH = 555.876
        GR_ORDER = 1
        CEN_PIX  = 367
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 312
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (29,30) pixels <8378>
    W_WIDTH  = 29
    W_HEIGHT = 30
    VDS_BACK = 1
    LL_ID    = 214
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = WW_552_72                               
        WIN_DEF  = (326,437,29,30)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_555_88                               
        WIN_DEF  = (353,437,29,30)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (596,437,29,30)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (983,437,29,30)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 1
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(15,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 15
    NY       = 1

RASTER_VAR
    RAS_ID   = 1
    RAS_VAR  = 13
    RV_DESC  = (30x60) arcsec, 3s <QUIET>  Comp. 2 IDs-(214,312)
    EXPTIME  = 3
    LL_ID    = 214
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 312
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 105
    USABLE   = Y

STUDY
    STUDY_ID = 5
    TITLE_ID = 387
    OBS_PROG = G_SPIC_1
    TITLE    = GARCHING FAST SPICULE STUDY - 2" SLIT
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 1
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 5
    TITLE_ID = 387
    STUDYVAR = 17
    SV_DESC  = VARIATION 1,  3 SEC EXPOSURE
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 105
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 1
        RAS_VAR  = 13
        N_REPEAT_R = 1
