DATATYPE = CDS STUDY DEFINITION
FILENAME = helium_3.def
INSTRUME = CDS
DATE_CRE = 1997/03/18 11:39:15
END

LINELIST
    LL_ID    = 180
    DETECTOR = N
    LL_DESC  = Helen Line List 2
    N_LINES  = 15
    LL_IND   = 1
        LINENAME = O III
        WAVELNTH = 525.796
        GR_ORDER = 1
        CEN_PIX  = 109
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 537.035
        GR_ORDER = 1
        CEN_PIX  = 206
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Ne IV
        WAVELNTH = 543.892
        GR_ORDER = 1
        CEN_PIX  = 264
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O IV
        WAVELNTH = 554.2
        GR_ORDER = 1
        CEN_PIX  = 353
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O IV
        WAVELNTH = 555.263
        GR_ORDER = 1
        CEN_PIX  = 362
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Ne V
        WAVELNTH = 572.331
        GR_ORDER = 1
        CEN_PIX  = 508
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = He I
        WAVELNTH = 584.327
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 9
        LINENAME = O III
        WAVELNTH = 599.597
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 10
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O IV
        WAVELNTH = 608.397
        GR_ORDER = 1
        CEN_PIX  = 815
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = Mg X
        WAVELNTH = 609.793
        GR_ORDER = 1
        CEN_PIX  = 827
        WAVEBAND = 2
    LL_IND   = 13
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 15
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 249
    DETECTOR = N
    DW_DESC  = Background,  15 lines. {0}  dex = (30,120) pixels <21004>
    W_WIDTH  = 30
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 180
    N_WINS   = 19
    DW_IND   = 1
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (94,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_537_03                             
        WIN_DEF  = (191,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Ne_4_543_89                             
        WIN_DEF  = (249,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_4_554_20                              
        WIN_DEF  = (338,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_4_555_26                              
        WIN_DEF  = (347,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (411,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Ne_5_572_33                             
        WIN_DEF  = (493,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (595,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = O_3_599_60                              
        WIN_DEF  = (725,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (793,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_4_608_40                              
        WIN_DEF  = (800,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = Mg_10_609_79                            
        WIN_DEF  = (812,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (847,512,30,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (941,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (982,392,30,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 21
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(20,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 21
    RAS_VAR  = 4
    RV_DESC  = (40x240) arcsec, 70s <QUIET>  Comp. 2 IDs-(180,249)
    EXPTIME  = 70
    LL_ID    = 180
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 249
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 1556
    USABLE   = Y

STUDY
    STUDY_ID = 23
    TITLE_ID = 346
    OBS_PROG = HELIUM
    TITLE    = HELIUM ENHANCEMENT STUDY
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 21
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 23
    TITLE_ID = 346
    STUDYVAR = 3
    SV_DESC  = OXFORD VARIATION
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1556
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 21
        RAS_VAR  = 4
        N_REPEAT_R = 1
